read_vtoc (3X) Miscellaneous Library Functions SunOS 5.5

NAME read_vtoc, write_vtoc − read and write a disk’s VTOC

SYNOPSIS #include <sys/vtoc.h> cc [ flag ... ] file ... − ladm [ library ... ] int read_vtoc(int fd, struct vtoc ∗vtoc);

int write_vtoc(int fd, struct vtoc ∗vtoc);

MT-LEVEL Unsafe

DESCRIPTION read_vtoc( ) returns the VTOC structure that is stored on the disk associated with the open file descriptor fd.

write_vtoc( ) stores the VTOC structure on at disk associated with the open file descriptor fd. fdrefers to any slice on a raw disk.

RETURN VALUES read_vtoc returns:

positive number Success. The positive number is the slice index associated with the open file descriptor.

negative number There are two possible error returns. VT_EIO indicates an

I/O error occurred and VT_ERROR indicates an unknown error.

write_vtoc returns:

0 Success negative number There are three possible error returns. VT_EIO indicates an I/O error occurred, VT_ERROR indicates an unknown error, and VT_EINVAL indicates an incorrect field within the VTOC.

SEE ALSO format (1M), fmthard (1M), prtvtoc (1M), ioctl (2), dkio (7I)

BUGS write_vtoc cannot write a VTOC on an unlabeled disk. Use format (1M) for this purpose.

3X-894 modified 22 Jan 1993