SunOS 5.5 Driver Entry Points identify (9E)

NAME identify − claim to drive a device

SYNOPSIS #include <sys/conf.h>

#include <sys/ddi.h>

#include <sys/sunddi.h> int prefixidentify(dev_info_t ∗dip);

INTERFACE

LEVEL Solaris DDI specific (Solaris DDI). This entry point is required . You must write it.

ARGUMENTS dip A pointer to a dev_info structure.

DESCRIPTION identify( ) determines whether this driver drives the device pointed to by dip.

RETURN VALUES identify( ) should return:

DDI_IDENTIFIED if it claims to drive this device.

DDI_NOT_IDENTIFIED if it does not claim to drive this device.

EXAMPLES #define XX_NAME "xx" static int xxidentify(dev_info_t ∗dip) { if (strcmp(ddi_get_name(dip), XX_NAME) == 0) {

/∗name matches device name∗/ return(DDI_IDENTIFIED);

}else return(DDI_NOT_IDENTIFIED); } SEE ALSO attach (9E), ddi_get_name (9F), strcmp (9F)

WritingDevice Drivers

WARNINGS This routine may be called multiple times. It may also be called at any time. The driver should not infer anything from the the sequence or the number of times this entry point has been called.

modified 11 Apr 1991 9E-27