SunOS 5.5 Driver Entry Points tran_getcap (9E)

NAME tran_getcap, tran_setcap − get/set SCSI transport capability

SYNOPSIS #include <sys/scsi/scsi.h> int prefixtran_getcap(struct scsi_address ∗ap, char ∗cap, int whom);

int prefixtran_setcap(struct scsi_address ∗ap, char ∗cap, int value, int whom);

INTERFACE

LEVEL Solaris architecture specific (Solaris DDI).

ARGUMENTS ap Pointer to the scsi_address (9S) structure.

cap Pointer to the string capability identifier.

value Defines the new state of the capability.

whom Specifies whether all targets or only the specified target is affected.

DESCRIPTION The tran_getcap( ) and tran_setcap( ) vectors in the scsi_hba_tran (9S) structure must be initialized during the HBA driver’s attach (9E) to point to HBA entry points to be called when a target driver calls scsi_ifgetcap (9F) and scsi_ifsetcap (9F).

tran_getcap( ) is called to get the current value of a capability specific to features provided by the HBA hardware or driver. The name of the capability cap is the NULL terminated capability string.

If whomis non-zero, the request is for the current value of the capability defined for the target specified by the scsi_address (9S) structure pointed to by ap; if whomis 0 all targets are affected, else the target specified by the scsi_address structure pointed to by ap is affected.

tran_setcap( ) is called to set the value of the capability cap to the value of value. If whom is non-zero, the capability should be set for the target specified by the scsi_address (9S) structure pointed to by ap; if whomis 0 all targets are affected, else the target specified by the scsi_address structure pointed to by ap is affected.

A device may support only a subset of the defined capabilities.

Refer to scsi_ifgetcap (9F) for the list of defined capabilities.

HBA drivers should use scsi_hba_lookup_capstr (9F) to match cap against the canonical capability strings.

RETURN VALUES tran_setcap( ) must return 1 if the capability was successfully set to the new value, 0 if the

HBA driver does not support changing the capability, and − 1 if the capability was not defined.

tran_getcap( ) must return the current value of a capability or − 1 if the capability was not defined.

SEE ALSO attach (9E), scsi_hba_attach (9F), scsi_hba_lookup_capstr (9F), scsi_ifgetcap (9F), scsi_address (9S), scsi_hba_tran (9S)

WritingDevice Drivers modified 30 Aug 1995 9E-57