tran_sync_pkt (9E) Driver Entry Points SunOS 5.5

NAME tran_sync_pkt − SCSI HBA memory synchronization entry point

SYNOPSIS #include <sys/scsi/scsi.h> void prefixtran_sync_pkt(struct scsi_address ∗ap, struct scsi_pkt ∗pkt);

INTERFACE

LEVEL Solaris architecture specific (Solaris DDI).

ARGUMENTS ap A pointer to a scsi_address (9S) structure.

pkt A pointer to a scsi_pkt (9S) structure.

DESCRIPTION The tran_sync_pkt( ) vector in the scsi_hba_tran (9S) structure must be initialized during the HBA driver’s attach (9E) to point to an HBA driver entry point to be called when a target driver calls scsi_sync_pkt (9F).

tran_sync_pkt( ) must synchronize a CPU’s or device’s view of the data associated with the pkt, typically by calling ddi_dma_sync (9F). The operation may also involve HBA hardware-specific details, such as flushing I/O caches, or stalling until hardware buffers have been drained.

SEE ALSO tran_init_pkt (9E), ddi_dma_sync (9F), scsi_hba_attach (9F), scsi_init_pkt (9F), scsi_sync_pkt (9F), scsi_hba_tran (9S), scsi_pkt (9S)

WritingDevice Drivers

NOTES A target driver may call tran_sync_pkt( ) on packets for which no DMA resources were allocated.

9E-66 modified 1 Nov 1993