Index A aread — asynchronous read from a device, 9E-13 asynchronous read — aread, 9E-13 asynchronous write — awrite, 9E-16 awrite — asynchronous write to a device, 9E-16 C character-oriented drivers

— ioctl, 9E-28 D DDI device mapping mapdev_access — device mapping access entry point, 9E-33 mapdev_dup — device mapping duplication entry point, 9E-35 mapdev_free — device mapping free entry point, 9E-36 dev_info structure convert device number to — getinfo, 9E-25 device access

— close, 9E-21

— open, 9E-41 device mapping access entry point — mapdev_access, 9E-33 device mapping duplication entry point — mapdev_dup, 9E-35 device mapping free entry point — mapdev_free,

9E-36 device number convert to dev_info structure — getinfo,

9E-25 devices attach to system — attach, 9E-15 claim to drive a device — identify, 9E-27 detach from system — detach, 9E-23 read data — read, 9E-49 write data to a device — write, 9E-70 devices, memory mapped check virtual mapping — mmap, 9E-37 devices, memory mapping map device memory into user space — segmap, 9E-50 devices, non-self-identifying determine if present — probe, 9E-44

Driver entry point routines

— _fini, 9E-10

— _info, 9E-10

— _init, 9E-10

— attach, 9E-15

— chpoll, 9E-18

— close, 9E-21

— detach, 9E-23

— dump, 9E-24

— getinfo, 9E-25

— identify, 9E-27

Driver entry point routines, continued

— ioctl, 9E-28

— mmap, 9E-37

— open, 9E-41

— print, 9E-43

— probe, 9E-44

— prop_op, 9E-45

— put, 9E-47

— read, 9E-49

— segmap, 9E-50

— srv, 9E-52

— strategy, 9E-54

— write, 9E-70 driver messages display on system console — print, 9E-43 driver property information report —prop_op, 9E-45 drivers, character-oriented

— ioctl, 9E-28 dump — dump memory to disk during system failure, 9E-24 dynamically update kstats — ks_update, 9E-31 G get/set SCSI transport capability — tran_getcap,

9E-57 tran_setcap, 9E-57 H HBA resources request to free HBA resources allocated on behalf of a target — tran_tgt_free, 9E-67 request to initialize HBA resources on behalf of a particular target — tran_tgt_init, 9E-68

I identify — claim to drive a device, 9E-27 K kernel modules, dynamic loading initialize a loadable module — _init, 9E-10 prepare loadable module for unloading —

_fini, kernel modules, dynamic loading, continued

9E-10 return loadable module information — _info,

9E-10 ks_update — dynamically update kstats, 9E-31 M mapdev_access — device mapping access entry point, 9E-33 mapdev_dup — device mapping duplication entry point, 9E-35 mapdev_free — device mapping free entry point,

9E-36 memory mapping for devices check virtual mapping — mmap, 9E-37 map device memory into user space — segmap, 9E-50 N non-self-identifying devices determine if present — probe, 9E-44 non-STREAMS character device driver poll entry point — chpoll, 9E-18 P put — receive messages from the preceding queue,

9E-47 R request to notify SCSI target of bus reset

— tran_reset_notify, 9E-62 reset a SCSI bus or target — tran_reset, 9E-61 S SCSI bus request to probe SCSI bus for a particular target

— tran_tgt_probe, 9E-69

SCSI command abort — tran_abort, 9E-55 request to transport — tran_start, 9E-63

SCSI HBA DMA deallocation entry point — tran_dmafree, 9E-56

SCSI HBA memory synchronization entry point — tran_sync_pkt, 9E-66

SCSI HBA packet preparation and deallocation — tran_init_pkt, 9E-58 tran_destroy_pkt, 9E-58 strategy — perform block I/O, 9E-54

STREAMS message queues receive messages from the preceding queue — put, 9E-47 service queued messages — srv, 9E-52 T

tran_abort — abort a SCSI command, 9E-55
tran_destroy_pkt — SCSI HBA packet preparation and deallocation, 9E-58 tran_dmafree — SCSI HBA DMA deallocation entry point, 9E-56 tran_getcap — get/set SCSI transport capability,

9E-57 tran_init_pkt — SCSI HBA packet preparation and deallocation, 9E-58 tran_reset — reset a SCSI bus or target, 9E-61
tran_reset_notify — request to notify SCSI target of bus reset, 9E-62 tran_setcap — get/set SCSI transport capability,

9E-57 tran_start — request to transport a SCSI command, 9E-63 tran_sync_pkt — SCSI HBA memory synchronization entry point, 9E-66 tran_tgt_free — request to free HBA resources allocated on behalf of a target, 9E-67 tran_tgt_init — request to initialize HBA resources on behalf of a particular target, 9E-68 tran_tgt_probe — request to probe SCSI bus for a particular target, 9E-69 V virtual address space dump portion of to disk in case of system failure — dump, 9E-24

W write — write data to a device, 9E-70