SunOS 5.5 Kernel Functions for Drivers bcmp (9F)

NAME bcmp − compare two byte arrays

SYNOPSIS #include <sys/types.h>

#include <sys/ddi.h> int bcmp(char ∗s1, char ∗ s2, size_t len);

INTERFACE

LEVEL Architecture independent level 1 (DDI/DKI).

ARGUMENTS s1 Pointer to the first character string.

s2 Pointer to the second character string.

len Number of bytes to be compared.

DESCRIPTION bcmp( ) compares two byte arrays of length len.

RETURN VALUES bcmp( ) returns 0 if the arrays are identical, or 1 if they are not.

CONTEXT bcmp( ) can be called from user or interrupt context.

SEE ALSO strcmp (9F)

WritingDevice Drivers

NOTES Unlike strcmp (9F), bcmp( ) does not terminate when it encounters a null byte.

modified 11 Apr 1991 9F-43