bzero (9F) Kernel Functions for Drivers SunOS 5.5

NAME bzero − clear memory for a given number of bytes

SYNOPSIS #include <sys/types.h>

#include <sys/ddi.h> void bzero(caddr_t addr, size_t bytes);

INTERFACE

LEVEL Architecture independent level 1 (DDI/DKI).

ARGUMENTS addr Starting virtual address of memory to be cleared.

bytes The number of bytes to clear starting at addr.

DESCRIPTION bzero( ) clears a contiguous portion of memory by filling it with zeros.

CONTEXT bzero( ) can be called from user or interrupt context.

SEE ALSO bcopy (9F), clrbuf (9F), kmem_zalloc (9F)

WritingDevice Drivers

WARNINGS The address range specified must be within the kernel space. No range checking is done.

If an address outside of the kernel space is selected, the driver may corrupt the system in an unpredictable way.

9F-58 modified 27 Jan 1993