SunOS 5.5 Kernel Functions for Drivers clrbuf (9F)

NAME clrbuf − erase the contents of a buffer

SYNOPSIS #include <sys/types.h>

#include <sys/buf.h> void clrbuf(struct buf ∗bp);

INTERFACE

LEVEL Architecture independent level 1 (DDI/DKI).

ARGUMENTS bp Pointer to the buf (9S) structure.

DESCRIPTION clrbuf( ) zeros a buffer and sets the b_resid member of the buf (9S) structure to 0. Zeros are placed in the buffer starting at bp->b_un.b_addr for a length of bp->b_bcount bytes.

b_un.b_addr and b_bcount are members of the buf (9S) data structure.

CONTEXT clrbuf( ) can be called from user or interrupt context.

SEE ALSO getrbuf (9F), buf (9S)

WritingDevice Drivers modified 27 Jan 1993 9F-61