dupmsg (9F) Kernel Functions for Drivers SunOS 5.5

NAME dupmsg − duplicate a message

SYNOPSIS #include <sys/stream.h> mblk_t ∗dupmsg(mblk_t ∗mp);

INTERFACE

LEVEL Architecture independent level 1 (DDI/DKI).

ARGUMENTS mp Pointer to the message.

DESCRIPTION dupmsg( ) forms a new message by copying the message block descriptors pointed to by mp and linking them. dupb (9F) is called for each message block. The data blocks themselves are not duplicated.

RETURN VALUES If successful, dupmsg( ) returns a pointer to the new message block. Otherwise, it returns a NULL pointer. A return value of NULL indicates either memory depletion or the data block reference count, db_ref (see datab (9S)), has reached a limit (255). See dupb (9F).

CONTEXT dupmsg( ) can be called from user, kernel, or interrupt context.

EXAMPLES See copyb (9F) for an example using dupmsg( ).

SEE ALSO copyb (9F), copymsg (9F), dupb (9F)

WritingDevice Drivers

STREAMSProgramming Guide

9F-232 modified 11 Apr 1991