putnext (9F) Kernel Functions for Drivers SunOS 5.5

NAME putnext − send a message to the next queue

SYNOPSIS #include <sys/stream.h>

#include <sys/ddi.h> int putnext(queue_t ∗q, mblk_t ∗mp);

INTERFACE

LEVEL Architecture independent level 1 (DDI/DKI).

ARGUMENTS q Pointer to the queue from which the message mp will be sent.

mp Message to be passed.

DESCRIPTION putnext( ) is used to pass a message to the put (9E) routine of the next queue in the stream.

RETURN VALUES None.

CONTEXT putnext( ) can be called from user or interrupt context.

EXAMPLE See allocb (9F) for an example of using putnext( ).

SEE ALSO allocb (9F), put (9E)

WritingDevice Drivers

STREAMSProgramming Guide

9F-298 modified 11 Apr 1991