scsi_abort (9F) Kernel Functions for Drivers SunOS 5.5

NAME scsi_abort − abort a SCSI command

SYNOPSIS #include <sys/scsi/scsi.h> int scsi_abort(struct scsi_address ∗ap, struct scsi_pkt ∗pkt);

INTERFACE

LEVEL Solaris DDI specific (Solaris DDI).

ARGUMENTS ap Pointer to a scsi_address structure.

pkt Pointer to a scsi_pkt (9S) structure.

DESCRIPTION scsi_abort( ) terminates a command that has been transported to the host adapter driver.

A NULL pkt causes all outstanding packets to be aborted. On a successful abort, the pkt_reason is set to CMD_ABORTED and pkt_statistics is OR’ed with STAT_ABORTED.

RETURN VALUES scsi_abort( ) returns:

1 on success.

0 on failure.

CONTEXT scsi_abort( ) can be called from user or interrupt context.

EXAMPLE if (scsi_abort(&devp->sd_address, pkt) == 0) {

(void) scsi_reset(&devp->sd_address, RESET_ALL); } SEE ALSO tran_abort (9E), scsi_reset (9F), scsi_pkt (9S)

WritingDevice Drivers

9F-328 modified 30 Aug 1995