scsi_poll (9F) Kernel Functions for Drivers SunOS 5.5

NAME scsi_poll − run a polled SCSI command on behalf of a target driver

SYNOPSIS #include <sys/scsi/scsi.h> int scsi_poll(struct scsi_pkt ∗pkt);

INTERFACE

LEVEL Solaris DDI specific (Solaris DDI).

ARGUMENTS pkt Pointer to the scsi_pkt (9S) structure.

DESCRIPTION scsi_poll( ) requests the host adapter driver to run a polled command. Unlike scsi_transport (9F) which runs commands asynchronously, scsi_poll( ) runs commands to completion before returning. If the pkt_time member of pkt is 0, the value of pkt_time is defaulted to SCSI_POLL_TIMEOUT to prevent an indefinite hang of the system.

RETURN VALUES scsi_poll( ) returns:

0 command completed successfully.

-1 command failed.

CONTEXT scsi_poll( ) can be called from user or interrupt level.

SEE ALSO makecom (9F), scsi_transport (9F), scsi_pkt (9S)

WritingDevice Drivers SH WARNINGS

Since scsi_poll( ) runs commands to completion before returning, it may require more time than is desirable when called from interrupt context. Therefore, calling scsi_poll from interrupt context is not recommended.

9F-358 modified 30 Aug 1995