SunOS 5.5 Kernel Functions for Drivers scsi_reset (9F)

NAME scsi_reset − reset a SCSI bus or target

SYNOPSIS #include <sys/scsi/scsi.h> int scsi_reset(struct scsi_address ∗ap, int level);

INTERFACE

LEVEL Solaris DDI specific (Solaris DDI).

ARGUMENTS ap Pointer to the scsi_address structure.

level The level of reset required.

DESCRIPTION scsi_reset( ) asks the host adapter driver to reset the SCSI bus or a SCSI target as specified by level. If levelequals RESET_ALL, the SCSI bus is reset. If it equals RESET_TARGET, ap is used to determine the target to be reset.

On a successful reset, the pkt_reason is set to CMD_RESET and pkt_statistics is OR’ed with STAT_BUS_RESET or STAT_DEV_RESET.

RETURN VALUES scsi_reset( ) returns:

1 on success.

0 on failure.

CONTEXT scsi_reset( ) can be called from user or interrupt context.

SEE ALSO tran_reset (9E), tran_reset_notify (9E), scsi_abort (9F)

WritingDevice Drivers modified 30 Aug 1995 9F-361