SunOS 5.5 Kernel Functions for Drivers unlinkb (9F)

NAME unlinkb − remove a message block from the head of a message

SYNOPSIS #include <sys/stream.h> mblk_t ∗unlinkb(mblk_t ∗mp);

INTERFACE

LEVEL Architecture independent level 1 (DDI/DKI).

ARGUMENTS mp Pointer to the message.

DESCRIPTION unlinkb( ) removes the first message block from the message pointed to by mp. A new message, minus the removed message block, is returned.

RETURN VALUES If successful, unlinkb( ) returns a pointer to the message with the first message block removed. If there is only one message block in the message, NULL is returned.

CONTEXT unlinkb( ) can be called from user or interrupt context.

EXAMPLE The routine expects to get passed an M_PROTO T_DATA_IND message. It will remove and free the M_PROTO header and return the remaining M_DATA portion of the message.

1 mblk_t ∗

2 makedata(mp)

3 mblk_t ∗mp; 4 { 5 mblk_t ∗nmp; 6 7 nmp = unlinkb(mp);

8 freeb(mp);

9 return(nmp);

10 }

SEE ALSO linkb (9F)

WritingDevice Drivers

STREAMSProgramming Guide modified 11 Apr 1991 9F-387