scsi_hba_init (9F) Kernel Functions for Drivers SunOS 5.5

NAME scsi_hba_init, scsi_hba_fini − SCSI Host Bus Adapter system initialization and completion routines

SYNOPSIS #include <sys/scsi/scsi.h> int scsi_hba_init(struct modlinkage ∗modlp);

void scsi_hba_fini(struct modlinkage ∗modlp);

INTERFACE

LEVEL Solaris architecture specific (Solaris DDI).

ARGUMENTS modlp Pointer to the Host Bus Adapters module linkage structure.

DESCRIPTION scsi_hba_init( ) scsi_hba_init( ) is the system-provided initialization routine for SCSI HBA drivers. The scsi_hba_init( ) function registers the HBA in the system and allows the driver to accept configuration requests on behalf of SCSI target drivers. The scsi_hba_init( ) routine must be called in the HBA’s _init (9E) routine before mod_install (9F) is called. If mod_install (9F) fails, the HBA’s _init (9E) should call scsi_hba_fini (9F) before returning failure.

scsi_hba_fini( ) scsi_hba_fini( ) is the system provided completion routine for SCSI HBA drivers.

scsi_hba_fini( ) removes all of the system references for the HBA that were created in scsi_hba_init( ). The scsi_hba_fini( ) routine should be called in the HBA’s _fini (9E) routine if mod_remove (9F) is successful.

RETURN VALUES scsi_hba_init( ) returns 0 if successful, and a non-zero value otherwise. If scsi_hba_init( ) fails, the HBA’s _init( ) entry point should return the value returned by scsi_hba_init( ).

CONTEXT scsi_hba_init( ) and scsi_hba_fini( ) should be called from _init (9E) or _fini (9E), respectively.

SEE ALSO _init (9E), _fini (9E), mod_install (9F), mod_remove (9F), scsi_pktfree (9F), scsi_pktalloc (9F), scsi_hba_tran (9S)

WritingDevice Drivers

NOTES The HBA is responsible for ensuring that no DDI request routines are called on behalf of its SCSI target drivers once scsi_hba_fini( ) is called.

9F-342 modified 1 Nov 1993