scsi_hba_probe (9F) Kernel Functions for Drivers SunOS 5.5

NAME scsi_hba_probe − default SCSI HBA probe function

SYNOPSIS #include <sys/scsi/scsi.h> int scsi_hba_probe(struct scsi_device ∗sd, int (∗waitfunc)(void));

INTERFACE

LEVEL Solaris architecture specific (Solaris DDI).

ARGUMENTS sd Pointer to a scsi_device (9S) structure describing the target.

waitfunc NULL_FUNC or SLEEP_FUNC .

DESCRIPTION scsi_hba_probe( ) is a function providing the semantics of scsi_probe (9F). An HBA driver may call scsi_hba_probe( ) from its tran_tgt_probe (9E) entry point, to probe for the existence of a target on the SCSI bus, or the HBA may set tran_tgt_probe (9E) to point to scsi_hba_probe directly.

RETURN VALUES See scsi_probe (9F) for the return values from scsi_hba_probe( ).

CONTEXT scsi_hba_probe( ) should only be called from the HBA’s tran_tgt_probe (9E) entry point.

SEE ALSO tran_tgt_probe (9E), scsi_device (9S), scsi_probe (9F)

WritingDevice Drivers

9F-346 modified 30 Aug 1995