Solaris XWindow System 3.5 User Commands xpr (1)

NAME xpr − print an Xwindow dump

SYNOPSIS xpr [ − device devtype] [ − scale scale] [ − height inches] [ − width inches] [ − left inches] [

− top inches] [ − header string ] [ − trailer string ] [ − landscape ] [ − portrait ] [ − plane number ] [ − gray ] [ − rv ] [ − compact ] [ − output filename ] [ − append filename ] [ − noff ] [

− split n ] [ − psfig ] [ − density dpi ] [ − cutoff level] [ − noposition ] [ − gamma correction ] [

− render algorithm ] [ − slide ] [ filename ]

DESCRIPTION xpr takes as input a window dump file produced by xwd (1) and formats it for output on

PostScript printers, the Digital LN03 or LA100, the IBM PP3812 page printer, the HP

LaserJet (or other PCL printers), or the HP PaintJet. If no file argument is given, the standard input is used. By default, xpr prints the largest possible representation of the window on the output page. Options allow the user to add headers and trailers, specify margins, adjust the scale and orientation, and append multiple window dumps to a single output file. Output is to standard output unless − output is specified.

Command Options

− device devtype

Specifies the device on which the file will be printed. Currently supported:

la100 Digital LA100 ljet HP LaserJet series and other monochrome PCL devices such as

ThinkJet, QuietJet, RuggedWriter, HP2560 series, and HP2930 series printers ln03 Digital LN03 pjet HP PaintJet (color mode) pjetxl HP HP PaintJet XLColor Graphics Printer (color mode) pp IBM PP3812 ps PostScript printer

The default is PostScript. -device lw (LaserWriter) is equivalent to -device ps and is provided only for backwards compatibility.

− scale scale

Affects the size of the window on the page. The PostScript, LN03, and HP printers are able to translate each bit in a window pixel map into a grid of a specified size. For example each bit might translate into a 3x3 grid. This would be specified by − scale 3. By default a window is printed with the largest scale that will fit onto the page for the specified orientation.

− height inches

Specifies the maximum height of the page.

− width inches

Specifies the maximum width of the page.

− left inches

Specifies the left margin in inches. Fractions are allowed. By default the window xpr (1) User Commands Solaris XWindow System 3.5 is centered in the page.

− top inches

Specifies the top margin for the picture in inches. Fractions are allowed.

− header string

Specifies a header string to be printed above the window.

− trailer string

Specifies a trailer string to be printed below the window.

− landscape

Forces the window to printed in landscape mode. By default a window is printed such that its longest side follows the long side of the paper.

− plane number

Specifies which bit plane to use in an image. The default is to use the entire image and map values into black and white based on color intensities.

− gray 2 | 3 | 4

Uses a simple 2x2, 3x3, or 4x4 gray scale conversion on a color image, rather than mapping to strictly black and white. This doubles, triples, or quadruples the effective width and height of the image.

− portrait

Forces the window to be printed in portrait mode. By default a window is printed such that its longest side follows the long side of the paper.

− rv Forces the window to be printed in reverse video.

− compact

Uses simple run-length encoding for compact representation of windows with lots of white pixels.

− output filename

Specifies an output file name. If this option is not specified, standard output is used.

− append filename

Specifies a filename previously produced by xpr to which the window is to be appended.

− noff When specified in conjunction with − append , the window will appear on the same page as the previous window.

− split n This option allows the user to split a window onto several pages. This might be necessary for very large windows that would otherwise cause the printer to overload and print the page in an obscure manner.

− psfig Suppress translation of the PostScript picture to the center of the page.

− densitydpi

Indicates what dot-per-inch density should be used by the HP printer.

− cutofflevel

Changes the intensity level where colors are mapped to either black or white for monochrome output on a LaserJet printer. The level is expressed as percentage of

Solaris XWindow System 3.5 User Commands xpr (1) full brightness. Fractions are allowed.

− noposition

This option causes header, trailer, and image positioning command generation to be bypassed for LaserJet, PaintJet and PaintJet XLprinters.

− gamma correction

This changes the intensity of the colors printed by PaintJet XLprinter. The correction is a floating point value in the range 0.00 to 3.00. Consult the operator’s manual to determine the correct value for the specific printer.

− render algorithm

This allows PaintJet XLprinter to render the image with the best quality versus performance tradeoff. Consult the operator’s manual to determine which algorithms are available.

− slide This option allows overhead transparencies to be printed using the PaintJet and

PaintJet XLprinters.

SEE ALSO xwd (1), xwud (1), X11(7)

LIMITATIONS The current version of xpr can generally print out on the LN03 most Xwindows that are not larger than two-thirds of the screen. For example, it will be able to print out a large

Emacs window, but it will usually fail when trying to print out the entire screen. The

LN03 has memory limitations that can cause it to incorrectly print very large or complex windows. The two most common errors encountered are ‘‘band too complex’’ and ‘‘page memory exceeded.’’ In the first case, a window may have a particular six pixel row that contains too many changes (from black to white to black). This will cause the printer to drop part of the line and possibly parts of the rest of the page. The printer will flash the number ‘1’on its front panel when this problem occurs. A possible solution to this problem is to increase the scale of the picture, or to split the picture onto two or more pages.

The second problem, ‘‘page memory exceeded,’’ will occur if the picture contains too much black, or if the picture contains complex half-tones such as the background color of a display. When this problem occurs the printer will automatically split the picture into two or more pages. It may flash the number ‘5’on its from panel. There is no easy solution to this problem. It will probably be necessary to either cut and paste, or to rework the application to produce a less complex picture.

There are several limitations on the LA100 support: the picture will always be printed in portrait mode, there is no scaling, and the aspect ratio will be slightly off.

Support for PostScript output currently cannot handle the -append , -noff or -split options.

The -compact option is only supported for PostScript output. It compresses white space but not black space, so it is not useful for reverse-video windows.

For color images, should map directly to PostScript image support.

xpr (1) User Commands Solaris XWindow System 3.5

HP PRINTERS If no − densityis specified on the command line 300 dots per inch will be assumed for ljet and 90 dots per inch for pjet. Allowable densityvalues for a LaserJet printer are 300, 150,

100, and 75 dots per inch. Consult the operator’s manual to determine densities supported by other printers.

If no − scale is specified the image will be expanded to fit the printable page area.

The default printable page area is 8x10.5 inches. Other paper sizes can be accommodated using the − height and − width options.

Note that a 1024x768 image fits the default printable area when processed at 100 dpi with scale=1, the same image can also be printed using 300 dpi with scale=3 but will require considerably more data be transferred to the printer.

xpr may be tailored for use with monochrome PCL printers other than the LaserJet. To print on a ThinkJet (HP2225A) xpr could be invoked as:

xpr -density 96 -width 6.667 filename or for black-and-white output to a PaintJet:

xpr -density 180 filename

The monochrome intensity of a pixel is computed as 0.30∗R + 0.59∗G + 0.11∗B. If a pixel’s computed intensity is less than the − cutoff level it will print as white. This maps light-on-dark display images to black-on-white hardcopy. The default cutoff intensity is

50% of full brightness. Example: specifying − cutoff 87.5 moves the white/black intensity point to 87.5% of full brightness.

A LaserJet printer must be configured with sufficient memory to handle the image. For a full page at 300 dots per inch approximately 2MB of printer memory is required.

Color images are produced on the PaintJet at 90 dots per inch. The PaintJet is limited to sixteen colors from its 330 color palette on each horizontal print line. xpr will issue a warning message if more than sixteen colors are encountered on a line. xpr will program the PaintJet for the first sixteen colors encountered on each line and use the nearest matching programmed value for other colors present on the line.

Specifying the − rv, reverse video, option for the PaintJet will cause black and white to be interchanged on the output image. No other colors are changed.

Multiplane images must be recorded by xwdin ZPixmapformat. Single plane (monochrome) images may be in either XYPixmapor ZPixmapformat.

Solaris XWindow System 3.5 User Commands xpr (1)

Some PCL printers do not recognize image positioning commands. Output for these printers will not be centered on the page and header and trailer strings may not appear where expected.

The − gamma and -render options are supported only on the PaintJet XLprinters.

The − slide option is not supported for LaserJet printers.

The − split option is not supported for HP printers.

The − gray option is not supported for HP or IBM printers.

COPYRIGHT Copyright 1988, Massachusetts Institute of Technology.

Copyright 1986, Marvin Solomon and the University of Wisconsin.

Copyright 1988, Hewlett Packard Company.

See X11(7) for a full statement of rights and permissions.

AUTHORS Michael R. Gretzinger, MIT Project Athena, Jose Capo, MIT Project Athena (PP3812 support), Marvin Solomon, University of Wisconsin, Bob Scheifler, MIT, Angela Bock and E.

Mike Durbin, Rich Inc. (grayscale), Larry Rupp, HP (HP printer support).