spray (1M ) Maintenance Commands SunOS 5.5

NAME spray − spray packets

SYNOPSIS /usr/sbin/spray [ − c count ] [ − d delay] [ − l length ] [ − t nettype ] host

AVAILABILITY SUNWcsu

DESCRIPTION spray sends a one-way stream of packets to host using RPC, and reports how many were received, as well as the transfer rate. The host argument can be either a name or an Internet address.

spray is not useful as a networking benchmark as it uses unreliable connectionless transports, (upd for example). spray can report a large number of packets dropped when the drops were caused by spray sending packets faster than they can be buffered locally

(before the packets get to the network medium).

OPTIONS − c count Specify how many packets to send. The default value of count is the number of packets required to make the total stream size 100000 bytes.

− d delay Specify how many microseconds to pause between sending each packet.

The default is 0.

− l length The length parameter is the numbers of bytes in the Ethernet packet that holds the RPC call message. Since the data is encoded using XDR, and

XDR only deals with 32 bit quantities, not all values of length are possible, and spray rounds up to the nearest possible value. When length is greater than 1514, then the RPC call can no longer be encapsulated in one

Ethernet packet, so the length field no longer has a simple correspondence to Ethernet packet size. The default value of length is 86 bytes (the size of the RPC and UDP headers).

− t nettype Specify class of transports. Defaults to netpath . See rpc(3N) for a description of supported classes.

SEE ALSO rpc(3N)

1M-618 modified 14 Sep 1992