SunOS 5.5 Maintenance Commands sttydefs (1M )

NAME sttydefs − maintain line settings and hunt sequences for TTYports

SYNOPSIS /usr/sbin/sttydefs − a ttylabel [ − b ] [ − f final-flags ] [ − i initial-flags ] [ − n nextlabel ]

/usr/sbin/sttydefs − l [ ttylabel ]

/usr/sbin/sttydefs − r ttylabel

AVAILABILITY SUNWcsu

DESCRIPTION sttydefs is an administrative command that maintains the line settings and hunt sequences for the system’s TTYports by making entries in, and deleting entries from the

/etc/ttydefs file.

sttydefs with a − a or − r option may be invoked only by the super-user. sttydefs with − l may be invoked by any user on the system.

OPTIONS − a ttylabel Add a record to the ttydefs file, using ttylabel as its label. The following describes the effect of the − b, − n, − i, or − f options when used in conjunction with the − a option:

− b Enable autobaud. Autobaud allows the system to set the line speed of a given TTYport to the line speed of the device connected to the port without the user’s intervention.

− f final-flags Specify the value to be used in the final-flags field in /etc/ttydefs . finalflags must be in a format recognized by the stty command. final-flags are the termio(7I) settings used by ttymon after receiving a successful connection request and immediately before invoking the service on the port.

If this option is not specified, sttydefs will set final-flags equal to the termio(7I) flags 9600 and sane .

− i initial-flags Specify the value to be used in the initial-flags field in /etc/ttydefs .

initial-flags must be in a format recognized by the stty command. These flags are used by ttymon when searching for the correct baud rate. They are set prior to writing the prompt.

If this option is not specified, sttydefs will set initial-flags equal to the termio(7I) flag 9600.

− n nextlabel Specify the value to be used in the nextlabel field in /etc/ttydefs . If this option is not specified, sttydefs will set nextlabel equal to ttylabel.

− l If a ttylabel is specified, sttydefs displays the record from /etc/ttydefs whose TTYlabel matches the specified ttylabel. If no ttylabel is specified, sttydefs displays the entire contents of /etc/ttydefs . sttydefs verifies that each entry it displays is correct and that the entry’s nextlabel field references an existing

− r ttylabel Remove any record in the ttydefs file that has ttylabel as its label.

modified 14 Sep 1992 1M-631 sttydefs (1M ) Maintenance Commands SunOS 5.5

OUTPUT If successful, sttydefs will exit with a status of 0. sttydefs − l will generate the requested information and send it to standard output.

EXAMPLES The following command lists all the entries in the ttydefs file and prints an error message for each invalid entry that is detected.

example# sttydefs − l

The following shows a command that requests information for a single label and its output:

example# sttydefs − l 9600

------------------------------------------------------------------

9600:9600 hupcl erase ^h:9600 sane ixany tab3 hupcl erase ^h::4800

------------------------------------------------------------------ ttylabel: 9600 initial flags: 9600 hupcl erase ^h final flags: 9600 sane ixany tab3 hupcl erase ^h autobaud: no nextlabel: 4800

The following sequence of commands will add the labels 1200, 2400, 4800, and 9600 and put them in a circular list:

sttydefs − a 1200 − n 2400 − i 1200 − f "1200 sane" sttydefs − a 2400 − n 4800 − i 2400 − f "2400 sane" sttydefs − a 4800 − n 9600 − i 4800 − f "4800 sane" sttydefs − a 9600 − n 1200 − i 9600 − f "9600 sane"

FILES /etc/ttydefs

SEE ALSO termio(7I)

1M-632 modified 14 Sep 1992