cg14config (1M ) Maintenance Commands SunOS 5.5

NAME cg14config − configure the cgfourteen device

SYNOPSIS /usr/platform/ platform-name/sbin/cg14config [ − d device] [ − r resolution ]

[ − g gammavalue ] [ − G gammafile ] [ − u degammavalue] [ − U degammafile]

AVAILABILITY SUNWkvm

DESCRIPTION cg14config sets up state on the selected cgfourteen device. platform-name can be found using the − i option of uname (1).

cg14config is supported only on Desktop SPARCsystems with SXgraphics option.

The interface, output, and command location are uncommitted and subject to change in future releases.

OPTIONS − d device Use deviceas the cgfourteen device to configure. Default is /dev/fb .

− r resolution Use resolution as the desired screen resolution. Resolution is specified in terms of screen width and height (in pixels), and vertical refresh (in hz).

Available resolutions are:

1024x768@60

1024x768@66

1024x768@70

1152x900@66

1152x900@76

1280x1024@66

1280x1024@76

1600x1280@66

1920x1080@72

The default is the value read from the monitor sense codes. Note that some or all of the resolutions above may not be supported by any given monitor. If a programmed resolution is outside of the range of allowable values for a monitor, unpredictable results can occur, including damage to the monitor. Thus, care should be taken when programming the resolution. See Openboot Command Referencefor a description of how to reset the console device to the default value if it becomes unusable from programming an unsupported resolution.

The − r option is not available when the window system is running.

− g gammavalue Each entry of the gamma lookup table will be loaded with entry^(1/ gammavalue). The gamma lookup table has 256 entries. Default gammavalue is 2.2.

− G filename Initialize the gamma lookup table with the contents of filename. The format of filename is 256 triplets (red green blue) of non-negative integers separated by NEWLINE characters. The integers must be in the range 0 to 1023, inclusive.

1M-106 modified 19 Apr 1995

SunOS 5.5 Maintenance Commands cg14config (1M )

− u degammavalue

Each entry of the degamma lookup table will be loaded with entry^( degammavalue). The degamma lookup table has 256 entries.

Default degammavalueis 2.2.

− U filename Initialize the degamma lookup table with the contents of filename. The format of filename is 256 entries of non-negative integers separated by

NEWLINE characters. The integers must be in the range 0 to 255, inclusive.

EXIT STATUS cg14config returns 0 on success and a positive integer on failure.

1 Selected device is not a cgfourteen device.

2 Requested action failed.

3 Unsupported resolution.

4 Gamma or degamma value out of range.

FILES /platform/ platform-name/kernel/drv/cgfourteen cgfourteen device driver

SEE ALSO uname (1), init (1M), mmap (2)

Platform Notes: SPARCstation 10SX System Configuration Guide

Openboot Command Reference modified 19 Apr 1995 1M-107