dminfo (1M ) Maintenance Commands SunOS 5.5

NAME dminfo − report information about a device entry in a device maps file

SYNOPSIS dminfo [ − v ] [ − a ] [ − f pathname ] dminfo [ − v ] [ − a ] [ − f pathname ] − n dev− name ...

dminfo [ − v ] [ − a ] [ − f pathname ] − d dev− path ...

dminfo [ − v ] [ − a ] [ − f pathname ] − t dev− type ...

dminfo [ − v ] [ − f pathname ] − u dm− entry

AVAILABILITY The functionality described in this man page is available only if the Basic Security

Module (BSM) has been enabled. See bsmconv (1M) for more information.

DESCRIPTION dminfo reports and updates information about the device_maps (4) file.

OPTIONS − v Verbose. Print the requested entry or entries, one line per entry, on the standard output. If no entries are specified, all are printed.

− a Succeed if any of the requested entries are found. If used with − v, all entries that match the requested case(s) are printed.

− f pathname Use a device_maps file with pathname instead of

/etc/security/device_maps .

− n dev− name Search by dev− name. Search device_maps (4) for a device_namefield matching dev− name. This option cannot be used with − d, − t or − u.

− d dev− path Search by dev− path. Search device_maps (4) for a device special pathname in the device_listfield matching the dev− path argument. This option cannot be used with − n, − t or − u.

− t dev− type Search by dev− type. Search device_maps (4) for a device_typefield matching the given dev− type. This option cannot be used with − d, − n or − u.

− u dm− entry Update the device_maps (4) file. This option is provided to add entries to the device_maps (4) file. The dm− entry must be a complete device_maps (4) file entry. The dm− entry has fields, as in the device_maps file. It uses the colon (:) as a field separator, and white space as the device_listsubfield separators. The dm− entry is not made if any fields are missing, or if the dm− entry would be a duplicate. The default device maps file can be updated only by the super user.

DIAGNOSTICS dminfo returns an exit code of 0 if successful, 1 if the request failed, and 2 if the invocation syntax was incorrect.

1M-166 modified 6 May 1993

SunOS 5.5 Maintenance Commands dminfo (1M )

FILES /etc/security/device_maps

SEE ALSO bsmconv (1M), device_maps (4) modified 6 May 1993 1M-167