NAME eeprom − EEPROM display and load utility

SYNOPSIS /usr/platform/ platform-name/sbin/eeprom [− ] [− f device] [parameter [=value] ...]

AVAILABILITY SPARC

SUNWcsu eeprom is only available on OpenBoot-compatible SPARC systems

DESCRIPTION eeprom displays or changes the values of parameters in the EEPROM. It processes parameters in the order given. When processing a parameter accompanied by a value, eeprom makes the indicated alteration to the EEPROM; otherwise it displays the parameter’s value.

When given no parameter specifiers, eeprom displays the values of all EEPROM parameters. A ‘− ’(hyphen) flag specifies that parameters and values are to be read from the standard input (one parameter or parameter=value per line).

Only the super-user may alter the EEPROM contents.

eeprom verifies the EEPROM checksums and complains if they are incorrect.

platform-name is the name of the platform implementation and can be found using the − i option of uname (1).

OPTIONS − f device Use deviceas the EEPROM device.

NVRAM

CONFIGURATION

PARAMETERS Not all OpenBoot systems support all parameters. Defaults may vary depending on the system and the PROM revision.

auto-boot? If true , boot automatically after power-on or reset. Defaults to true .

ansi-terminal? Configuration variable used to control the behavior of the terminal emulator. The value false makes the terminal emulator stop interpreting ANSI escape sequences, instead just echoing them to the output device. Default value: true .

boot-command Command executed if auto-boot? is true . Default value is boot .

boot-device Device from which to boot. Defaults to disk net .

boot-file File to boot (an empty string lets the secondary booter choose default). Defaults to empty string.

boot-from Boot device and file (OpenBoot PROM version 1.x only).

Defaults to vmunix.

boot-from-diag Diagnostic boot device and file (OpenBoot PROM version 1.x only). Defaults to le( )unix .

diag-device Diagnostic boot source device. Defaults to net .

diag-file File from which to boot in diagnostic mode. Defaults to empty string.

modified 5 Jul 1995 1M-175 eeprom (1M ) Maintenance Commands SunOS 5.5 diag-level Diagnostics level. Values include off, min , max and menus .

There may be additional platform-specific values. When set to off, POST is not called. If POST is called, the value is made available as an argument to, and is interpreted by

POST. The default value is platform-dependent .

diag-switch? If true , run in diagnostic mode. Defaults to true .

fcode-debug? If true , include name parameter for plug-in device FCodes.

Defaults to false .

hardware-revision System version information.

input-device Power-on input device (usually keyboard , ttya , or ttyb ).

Defaults to keyboard .

keyboard-click? If true enable keyboard click. Defaults to false .

keymap Keymap for custom keyboard.

last-hardware-update System update information.

load-base Default load address for client programs. Default value is

16384.

local-mac-address? If true, network drivers use their own MAC address, not system’s. Defaults to false .

mfg-mode Manufacturing mode argument for POST. Possible values include off or chamber . The value is passed as an argument to POST. Default value: off.

mfg-switch? If true, repeat system self-tests until interrupted with STOP-

A. Defaults to false .

nvramrc Contents of NVRAMRC . Defaults to empty.

oem-banner Custom OEM banner (enabled by setting oem-banner? to true ). Defaults to empty string.

oem-banner? If true , use custom OEM banner. Defaults to false .

oem-logo Byte array custom OEM logo (enabled by setting oem-logo?

to true ). Displayed in hexadecimal.

oem-logo? If true , use custom OEM logo (else, use Sun logo). Defaults to false .

output-device Power-on input device (usually screen , ttya , or ttyb ).

Defaults to screen .

sbus-probe-list Which SBus slots are probed and in what order. Defaults to

0123.

screen-#columns Number of on-screen columns (characters/line). Defaults to 80. screen-#rows Number of on-screen rows (lines). Defaults to 34.

scsi-initiator-id SCSI bus address of host adapter, range 0-7. Defaults to 7.

1M-176 modified 5 Jul 1995 sd-targets Map SCSI disk units (OpenBoot PROM version 1.x only).

Defaults to 31204567, which means that unit 0 maps to target

3, unit 1 maps to target 1, and so on.

security-#badlogins Number of incorrect security password attempts.

security-mode Firmware security level (options: none , command, or full ).

If set to command or full , system will prompt for PROM security password. Defaults to none .

security-password Firmware security password (never displayed). Can be set only when security-mode is set to command or full .

example# eeprom security-password=

Changing PROM password:

New password:

Retype new password:

selftest-#megs Metabytes of RAM to test. Ignored if diag-switch? is true .

Defaults to 1.

skip-vme-loopback? If true , POST does not do VMEbus loopback tests. Defaults to false .

st-targets Map SCSI tape units (OpenBoot PROM version 1.x only).

Defaults to 45670123, which means that unit 0 maps to target

4, unit 1 maps to target 5, and so on.

sunmon-compat? If true , display Restricted Monitor prompt (>). Defaults to false .

testarea One-byte scratch field, available for read/write test. Defaults to 0.

tpe-link-test? Enable 10baseT link test for built-in twisted pair Ethernet.

Defaults to true .

ttya-mode TTYA (baud rate, #bits, parity, #stop, handshake).

Defaults to 9600,8,n,1,− .

Fields, in left-to-right order, are:

baud rate: 110, 300, 1200, 4800, 9600...

data bits: 5, 6, 7, 8 parity: n(none), e(even), o(odd), m(mark), s(space) stop bits: 1, 1.5, 2 handshake: − (none), h(hardware:rts/cts), s(software:xon/xoff) modified 5 Jul 1995 1M-177 eeprom (1M ) Maintenance Commands SunOS 5.5 ttyb-mode TTYB(baud rate, #bits, parity, #stop, handshake).

Defaults to 9600,8,n,1,− .

Fields, in left-to-right order, are:

baud rate: 110, 300, 1200, 4800, 9600...

data bits: 5, 6, 7, 8 stop bits: 1, 1.5, 2 parity: n(none), e(even), o(odd), m(mark), s(space) handshake: − (none), h(hardware:rts/cts), s(software:xon/xoff) ttya-ignore-cd If true , operating system ignores carrier-detect on TTYA.

Defaults to true .

ttyb-ignore-cd If true , operating system ignores carrier-detect on TTYA.

Defaults to true .

ttya-rts-dtr-off If true , operating system does not assert DTR and RTS on

TTYA. Defaults to false .

ttyb-rts-dtr-off If true , operating system does not assert DTR and RTS on

TTYB. Defaults to false .

use-nvramrc? If true , execute commands in NVRAMRC during system start-up. Defaults to false .

version2? If true , hybrid (1.x/2. x) PROM comes up in version 2.x.

Defaults to true .

watchdog-reboot? If true , reboot after watchdog reset. Defaults to false .

EXAMPLES The following example demonstrates the method for changing from one to two the number of megabytes of RAM that the system will test.

example# eeprom selftest-#megs selftest-#megs=1 example# eeprom selftest-#megs=2 example# eeprom selftest-#megs selftest-#megs=2

The following example demonstrates the method for setting the auto-boot? parameter to true .

example# eeprom auto-boot?=true

When the eeprom command is executed in user mode, the parameters with a trailing question mark (?) need to be enclosed in double quotation marks (" ") to prevent the shell from interpreting the question mark. Preceding the question mark with an escape character (\ ) will also prevent the shell from interpreting the question mark.

1M-178 modified 5 Jul 1995 example% eeprom "auto-boot?"=true

FILES /dev/openprom device file

/usr/platform/ platform-name/sbin/eeprom platform-specific version of eeprom . To obtain platformname, use uname − i.

SEE ALSO passwd (1), sh(1), uname (1) modified 5 Jul 1995 1M-179