diskscan (1M ) Maintenance Commands SunOS 5.5

NAME diskscan − perform surface analysis

SYNOPSIS diskscan [ − W ] [ − n ] [ − y ] raw_device

AVAILABILITY x86

SUNWcsu

DESCRIPTION diskscan is used by the system administrator to perform surface analysis on a portion of a hard disk. The disk portion may be a raw partition or slice; it is identified using its raw device name. By default, the specified portion of the disk is read (non-destructive) and errors reported on standard error. In addition, a progress report is printed on standard out. The list of bad blocks should be saved in a file and later fed into addbadsec (1M), which will remap them.

− W Causes diskscan to perform write and read surface analysis. This type of surface analysis is destructive and should be invoked with caution.

− n Causes diskscan to suppress linefeeds when printing progress information on standard out.

− y Causes diskscan to suppress the warning regarding destruction of existing data that is issued when − W is used.

FILES The raw device should be /dev/rdsk/c?t?d?[ps]? .

SEE ALSO fdisk (1M), fmthard (1M), addbadsec (1M)

1M-162 modified 31 May 1993