term (5) Headers, Tables, and Macros SunOS 5.5

NAME term − conventional names for terminals

DESCRIPTION Terminal names are maintained as part of the shell environment in the environment variable TERM (see sh(1), profile(4), and environ (5)). These names are used by certain commands (for example, tabs , tput , and vi) and certain functions (for example, see curses (3X)).

Files under /usr/share/lib/terminfo are used to name terminals and describe their capabilities. These files are in the format described in terminfo(4). Entries in terminfo source files consist of a number of comma-separated fields. To print a description of a terminal term, use the command infocmp − I term (see infocmp (1M)). White space after each comma is ignored. The first line of each terminal description in the terminfo database gives the names by which terminfo knows the terminal, separated by bar (| ) characters.

The first name given is the most common abbreviation for the terminal (this is the one to use to set the environment variable TERMINFO in $HOME/.profile ; see profile(4)), the last name given should be a long name fully identifying the terminal, and all others are understood as synonyms for the terminal name. All names but the last should contain no blanks and must be unique in the first 14 characters; the last name may contain blanks for readability.

Terminal names (except for the last, verbose entry) should be chosen using the following conventions. The particular piece of hardware making up the terminal should have a root name chosen, for example, for the AT&T 4425 terminal, att4425. This name should not contain hyphens, except that synonyms may be chosen that do not conflict with other names. Up to 8 characters, chosen from the set a through z and 0 through 9, make up a basic terminal name. Names should generally be based on original vendors rather than local distributors. A terminal acquired from one vendor should not have more than one distinct basic name. Terminal sub-models, operational modes that the hardware can be in, or user preferences should be indicated by appending a hyphen and an indicator of the mode. Thus, an AT&T 4425 terminal in 132 column mode is att4425− w. The following suffixes should be used where possible:

Suffix Meaning Example

− w Wide mode (more than 80 columns) att4425−− w

− am With auto. margins (usually default) vt100− am

− nam Without automatic margins vt100− nam

− n Number of lines on the screen aaa−− 60

− na No arrow keys (leave them in local) c100− na

− np Number of pages of memory c100− 4p

− rv Reverse video att4415−− rv

To avoid conflicts with the naming conventions used in describing the different modes of a terminal (for example, − w), it is recommended that a terminal’s root name not contain hyphens. Further, it is good practice to make all terminal names used in the terminfo(4) database unique. Terminal entries that are present only for inclusion in other entries via the use= facilities should have a ’+’in their name, as in 4415+nl.

5-136 modified 3 Jul 1990

SunOS 5.5 Headers, Tables, and Macros term (5)

Here are some of the known terminal names: (For a complete list, enter the command ls -C /usr/share/lib/terminfo/? ).

2621,hp2621 Hewlett-Packard 2621 series

2631 Hewlett-Packard 2631 line printer

2631− c Hewlett-Packard 2631 line printer, compressed mode

2631− e Hewlett-Packard 2631 line printer, expanded mode

2640,hp2640 Hewlett-Packard 2640 series

2645,hp2645 Hewlett-Packard 2645 series

3270 IBM Model 3270

33,tty33 AT&T Teletype Model 33 KSR

35,tty35 AT&T Teletype Model 35 KSR

37,tty37 AT&T Teletype Model 37 KSR

4000a Trendata 4000a

4014,tek4014 TEKTRONIX 4014

40,tty40 AT&T Teletype Dataspeed 40/2

43,tty43 AT&T Teletype Model 43 KSR

4410,5410 AT&T 4410/5410 in 80-column mode, version 2

4410− nfk,5410−− nfk AT&T 4410/5410 without function keys, version 1

4410− nsl,5410 − nsl AT&T 4410/5410 without pln defined

4410− w,5410−− w AT&T 4410/5410 in 132-column mode

4410v1,5410v1 AT&T 4410/5410 in 80-column mode, version 1

4410v1− w,5410v1− w AT&T 4410/5410 in 132-column mode, version 1

4415,5420 AT&T 4415/5420 in 80-column mode

4415− nl,5420−− nl AT&T 4415/5420 without changing labels

4415− rv,5420− rv AT&T 4415/5420 80 columns in reverse video

4415− rv− nl,5420−− rv− nl AT&T 4415/5420 reverse video without changing labels

4415− w,5420−− w AT&T 4415/5420 in 132-column mode

4415− w−− nl,5420−− w−− nl AT&T 4415/5420 in 132-column mode without changing labels

4415− w−− rv,5420− w−− rv AT&T 4415/5420 132 columns in reverse video

4418,5418 AT&T 5418 in 80-column mode

4418− w,5418−− w AT&T 5418 in 132-column mode

4420 AT&T Teletype Model 4420

4424 AT&T Teletype Model 4424

4424-2 AT&T Teletype Model 4424 in display function group ii

4425,5425 AT&T 4425/5425

4425− fk,5425−− fk AT&T 4425/5425 without function keys modified 3 Jul 1990 5-137 term (5) Headers, Tables, and Macros SunOS 5.5

4425− nl,5425−− nl AT&T 4425/5425 without changing labels in

80-column mode

4425− w,5425−− w AT&T 4425/5425 in 132-column mode

4425− w−− fk,5425−− w−− fk AT&T 4425/5425 without function keys in

132-column mode

4425− nl−− w,5425−− nl−− w AT&T 4425/5425 without changing labels in

132-column mode

4426 AT&T Teletype Model 4426S

450 DASI 450 (same as Diablo 1620)

450− 12 DASI 450 in 12-pitch mode

500,att500 AT&T-IS 500 terminal

510,510a AT&T 510/510a in 80-column mode

513bct,att513 AT&T 513 bct terminal

5320 AT&T 5320 hardcopy terminal

5420_2 AT&T 5420 model 2 in 80-column mode

5420_2− w AT&T 5420 model 2 in 132-column mode

5620,dmd AT&T 5620 terminal 88 columns

5620− 24,dmd−− 24 AT&T Teletype Model DMD 5620 in a 24x80 layer

5620− 34,dmd−− 34 AT&T Teletype Model DMD 5620 in a 34x80 layer

610,610bct AT&T 610 bct terminal in 80-column mode

610− w,610bct − w AT&T 610 bct terminal in 132-column mode

630,630MTG AT&T 630 Multi-Tasking Graphics terminal

7300,pc7300,unix_pc AT&T UNIX PC Model 7300

735,ti Texas Instruments TI735 and TI725

745 Texas Instruments TI745 dumb generic name for terminals that lack reverse line-feed and other special escape sequences hp Hewlett-Packard (same as 2645) lp generic name for a line printer pt505 AT&T Personal Terminal 505 (22 lines) pt505−− 24 AT&T Personal Terminal 505 (24-line mode) sync generic name for synchronous Teletype

Model 4540-compatible terminals

Commands whose behavior depends on the type of terminal should accept arguments of the form − Tterm where term is one of the names given above; if no such argument is present, such commands should obtain the terminal type from the environment variable

TERM, which, in turn, should contain term.

FILES /usr/share/lib/terminfo/?/ ∗ compiled terminal description database

SEE ALSO sh(1), stty (1), tabs (1), tput (1), vi(1), infocmp (1M), curses (3X),profile(4), terminfo(4), environ (5)

5-138 modified 3 Jul 1990