bwtwo (7D ) Devices SunOS 5.5

NAME bwtwo − black and white memory frame buffer

SYNOPSIS /dev/fbs/bwtwo

DESCRIPTION The bwtwo interface provides access to monochrome memory frame buffers. It supports the ioctls described in fbio (7I).

Reading or writing to the frame buffer is not allowed — you must use the mmap (2) system call to map the board into your address space.

FILES /dev/fbs/bwtwo[0-9] device files

SEE ALSO mmap (2), cgfour (7D), fbio (7I)

BUGS Use of vertical-retrace interrupts is not supported.

7D-52 modified 27 Mar 1992