cgtwo (7D ) Devices SunOS 5.5

NAME cgtwo − color graphics interface

SYNOPSIS /dev/cgtwo n

DESCRIPTION The cgtwo interface provides access to the color graphics controller board, which is normally supplied with a 19’’66 Hz non-interlaced color monitor. It provides the standard frame buffer interface as defined in fbio (7I).

The hardware consumes 4 megabytes of VME bus address space. The board starts at standard address 0x400000. The board must be configured for interrupt level 4.

FILES /dev/cgtwo[0-9]

SEE ALSO mmap (2), fbio (7I)

7D-66 modified 21 Oct 1991