SunOS 5.5 Devices pcser (7D )

NAME pcser − PCMCIA serial card device driver

SYNOPSIS pcser@<socket>:pcser pcser@<socket>:pcser,cu

DESCRIPTION The PCMCIA serial card device driver supports asynchronous serial I/O access to any

PCMCIA card that that complies with Revision 2.1 of the PCMCIA Standard and which presents an 8250-type UART interface.

FILES /kernel/drv/pcser pcser driver

/dev/term/pc n dial-in devices

/dev/cua/pc n dial-out devices where:

n is the PCMCIA physical socket number.

SEE ALSO cu(1C), tip (1), uucp (1C), autopush (1M), pcmciad (1M), ports (1M), ioctl (2), open (2), pcmcia (4), ldterm (7M), termio(7I), ttcompat (7M)

DIAGNOSTICS pcser: socket n soft silo overflow

The driver’s character input ring buffer overflowed before it could be serviced.

pcser: socket n unable to get CIS information

The CIS on the card has incorrect information or is in an incorrect format.

This message usually indicates a non-compliant card.

modified 20 Mar 1995 7D-251