Index 1 1/2-inch tape drive xt — Xylogics 472

10/100 Mbit/s 802.30 Fast Ethernet device driver — be, 7D-40

3 3COM 3C503 Ethernet device driver — el, 7D-94

3COM 3C507 Ethernet device driver — elink,

7D-97

3COM EtherLink III Ethernet device driver — elx,

7D-100

3COM EtherLink III PCMCIA Ethernet Adapter — pcelx, 7D-239

4 450 SMD Disk driver — xy

451 SMD Disk driver — xy

472 1/2-inch tape drive — xt

4BSD compatibility module — ttcompat, 7M-384 7 7053 SMD Disk driver — xd

A Adaptec 154x ISA host bus adapter — aha, 7D-14

Adaptec 174x EISA host bus adapter — eha, 7D-93

Adaptec AHA-1510A based ISA host bus adapter module — aic, 7D-16

Adaptec AHA-1520A based ISA host bus adapter module — aic, 7D-16

Adaptec AHA-1522A based ISA host bus adapter module — aic, 7D-16

Adaptec AIC-6360 based ISA host bus adapter module — aic, 7D-16

Address Resolution Protocol, See ARP adp — low-level module for Adaptec 7870 based

SCSI controllers, 7D-13 aha — low-level module for Adaptec 154x ISA host bus adapter, 7D-14 aic — Adaptec AHA-1510A based ISA host bus adapter module, 7D-16

— Adaptec AHA-1520A based ISA host bus adapter module, 7D-16

— Adaptec AHA-1522A based ISA host bus adapter module, 7D-16

— Adaptec AIC-6360 based ISA host bus adapter module, 7D-16

ALM-2 Parallel Printer port driver — mcpp, 7D-203

ALM-2 Zilog 8530 SCC serial communications driver — mcpzsa

Am7990 (LANCE) Ethernet device driver

— le, 7D-186

— lebuffer, 7D-186

— ledma, 7D-186

Am79C940 (MACE) Ethernet device driver — qe,

7D-270 thru 7D-273

AMD PCnet Ethernet controller device driver — pcn, 7D-247

ANSI standard terminal emulation — wscons arp — Address Resolution Protocol, 7P-17 arp ioctl

   SIOCDARP — delete arp entry, 7P-17

   SIOCGARP — get arp entry, 7P-17

   SIOCSARP — set arp entry, 7P-17
asy — asynchronous serial port driver, 7D-20 asynchronous serial port driver — asy, 7D-20

AT attachment disk driver — ata, 7D-22 ata — AT attachment disk driver, 7D-22
audio — audio device interface, 7I-24 audio device

Sound Blaster 16 — sbpro, 7D-283

Sound Blaster AWE32 — sbpro, 7D-283

Sound Blaster Pro — sbpro, 7D-283 audioamd — telephone quality audio device, 7D-33
audiocs — Crystal Semiconductor 4231 audio

Interface, 7D-35

Audio Data Formats for the Multimedia 4231

Codec, 7D-35

Audio Interfaces, 7D-35

Audio Ports, 7D-36

Audio Status Change Notification, 7D-36

Sample Granularity, 7D-36 B

bd — SunButtons and SunDials STREAMS module,

7M-38 be — 10/100 Mbit/s 802.30 Fast Ethernet device driver, 7D-40 be and DLPI, 7D-40 be Primitives, 7D-40

BigMAC Ethernet device driver — be, 7D-40 bpp — bi-directional parallel port, 7D-43

                                             bufmod — STREAMS Buffer module, 7M-48 built-in mouse device interface — kdmouse,

7D-178 bwtwo — black and white frame buffer, 7D-52

C CD-ROM — ISO 9660 CD-ROM filesystem —

   hsfs, 7FS-125
cdio— CD-ROM control operations, 7I-53

CDROM control operations —cdio, 7I-53 cgfourteen — 24-bit color graphics device, 7D-63
cgeight — 24-bit color memory frame buffer,

7D-61 cgfour — P4-bus 8-bit color memory frame buffer,

7D-62 cgfourteen — 24-bit color graphics device, 7D-63
cgsix — accelerated 8-bit color frame buffer, 7D-64
cgthree — 8-bit color memory frame buffer, 7D-65
cgtwo — color graphics interface, 7D-66 change translation table entry ioctl — KIOCS-

   KEY, 7M-175
cmdk — common disk driver, 7D-67

Cogent EM100 Ethernet controller device driver — dnet, 7D-85

Cogent EM960 Ethernet controller device driver — dnet, 7D-85 color graphics interface

24-bit color memory frame buffer — cgeight,

7D-61

8-bit color memory frame buffer — cgthree,

7D-65 accelerated 8-bit color frame buffer — cgsix,

7D-64

— cgtwo, 7D-66

P4-bus 8-bit color memory frame buffer — cgfour, 7D-62

Sun color memory frame buffer — tcx,

7D-344 common disk driver — cmdk, 7D-67

Compaq Netflex-2 Ethernet device driver — nfe,

7D-231 connections, unique stream line discipline — connld, 7M-68 connld — line discipline for unique connections,

7M-68 console — STREAMS-based console interface,

7D-69 converts mouse protocol to Firm Events — vuidmice, 7M-397 vuid2ps2, 7M-397 vuid3ps2, 7M-397 vuidm3p, 7M-397 vuidm4p, 7M-397 vuidm5p, 7M-397 core memory image — mem, 7D-207 corvette — low-level module for IBM Micro

Channel SCSI-2 Fast/Wide Adapter/A, 7D-70

Crystal Semiconductor 4231 audio Interface —

   audiocs, 7D-35
csa — low-level module for Compaq SMART SCSI

Array Controller, 7D-71 D D-LINK Ethernet controller device driver — dnet,

7D-85

Data Link Provider Interface

— dlpi, 7P-84 dbri — ISDN and audio interface, 7D-72

Audio Data Formats for BRI Interfeces, 7D-73

Audio Data Formats for the Multimedia

Codec/SpeakerBox, 7D-73

Audio Interfaces, 7D-72

Audio Ports, 7D-74

Audio Status Change Notification, 7D-74

ISDN Interfaces, 7D-73

Sample Granularity, 7D-74 delete arp entry ioctl — SIOCDARP, 7P-17

Dell SCSI Array Controller (DSA) — dsa, 7D-88 device interface

Microsoft Bus Mouse — msm, 7D-214 devices cgfourteen, 7D-63 disk control operations — dkio, 7I-78 disk driver fd — floppy, 7D-111

disk driver, continued

Xylogics — xd, 7D-406 thru 7D-411 disk quotas — quotactl(), 7I-274 display — system console display, 7D-77
dkio — disk control operations, 7I-78

DKIOCEJECT — disk eject, 7I-78

DKIOCGAPART — get full disk partition table, 7I-78

DKIOCGGEOM — get disk geometry, 7I-78

DKIOCGVTOC — get volume table of contents (vtoc),

7I-78

DKIOCINFO — get disk controller info, 7I-78

DKIOCSAPART — set disk partition info, 7I-78

DKIOCSGEOM — set disk geometry, 7I-78

DKIOCSVTOC — set volume table of contents (vtoc),

7I-78 dlpi — Data Link Provider Interface, 7P-84
dnet — DEC 21040/21140-based Ethernet Controllers, 7D-85

— DOS formatted file system PCFS, 7FS-240 double-buffered 24-bit SBus color frame buffer and graphics accelerator — leo, 7D-190 dpt — DPT 2011, 2012, 2021, 2022, 2122, 2024, 2124,

3021, 3222, and 3224 controllers, 7D-87

DPT 2011, 2012, 2021, 2022, 2122, 2024, 2124, 3021,

3222, and 3224 controllers — dpt, 7D-87 driver for parallel port — lp, 7D-200 driver for SPARC Storage Array disk devices — ssd, 7D-302 drivers driver for SCSI disk devices — sd, 7D-285

SCSI tape devices — st, 7D-304 drivers for floppy disks and floppy disk controllers

— fd, 7D-111 fdc, 7D-111 dsa — low-level module for Dell SCSI Array Controller (DSA), 7D-88

Dual Basic Rate ISDN and audio Interface — dbri,

7D-72

E

eepro — EtherExpress-Pro Ethernet device driver,

7D-89 eha — low-level module for Adaptec 174x EISA host bus adapter, 7D-93 el — 3COM 3C503 Ethernet device driver, 7D-94
elink — 3COM 3C507 Ethernet device driver,

7D-97 elx — 3COM ETHERLINK III Ethernet device driver, 7D-100 elx Primitives, 7D-100 esa — low-level module for Adaptec 7770 based

SCSI controllers, 7D-103 esp — ESP SCSI Host Bus Adapter Driver, 7D-104

ESP SCSI Host Bus Adapter Driver — esp, 7D-104

EtherExpress 16 Ethernet device driver, Intel — iee, 7D-133

EtherExpress-Pro Ethernet device driver, Intel — eepro, 7D-89

Ethernet device driver

SMC 3032/EISA dual-channel Ethernet device driver — smce, 7D-292

SMC 8003/8013/8216/8416 Ethernet device driver — smc, 7D-289

SMC Elite32 Ultra (8232) Ethernet device driver

— smceu, 7D-295

SMC Ether100 (9232) Ethernet device driver — smcf, 7D-297

Ethernet driver — ie, 7D-130 F

fbio — frame buffer control operations, 7I-109
fd — drivers for floppy disks and floppy disk controllers, 7D-111 fdc — drivers for floppy disks and floppy disk controllers, 7D-111

FDGETCHANGE — get status of disk changed, 7I-116
fdio — disk control operations, 7I-116

FDIOGCHAR — get floppy characteristics, 7I-116

FDIOGCHAR — set floppy characteristics, 7I-116

FDKEJECT — eject floppy, 7I-116 file system

file system, continued quotactl() — disk quotas, 7I-274 floppy disk control operations — fdio, 7I-116 floppy disk driver — fd, 7D-111 frame buffer black and whirte frame buffer — bwtwo, 7D-52 frame buffer control operations

— fbio, 7I-109 G Generic LAN Driver — gld, 7D-120 get compatibility mode ioctl — KIOCGCOMPAT,

7M-177 get keyboard “direct input” state ioctl —

KIOCGDIRECT, 7M-177 get keyboard translation ioctl — KIOCGTRANS,

7M-175 get keyboard type ioctl — KIOCLAYOUT, 7M-176 get LEDs ioctl — KIOCGLED, 7M-177 get translation table entry ioctl — KIOCGKEY,

7M-176 gld — Generic LAN Driver, 7D-120 gld and Ethernet V2 and 802.3, 7D-120 gld and Style 1 and 2 Providers, 7D-121

Implemented DLPI Primitives, 7D-121 H

hdio — SMD and IPI disk control operations,

7I-123

High Sierra filesystem, See hsfs hsfs filesystem — hsfs, 7FS-125 I I/O data link provider interface — dlpi, 7P-84 extended terminal interface — termiox,

7I-364 ioctls that operate directly on sockets — sockio, 7I-301

STREAMS ioctl commands — streamio,

7I-326

IBM 16/4 Token Ring Network Adapter device driver — tr, 7D-379

IBM Micro Channel SCSI-2 Fast/Wide Adapter/A corvette — low-level module for, 7D-70

IBM MicroChannel host bus adapter

   mcis — low-level module for, 7D-202
icmp — Internet Control Message Protocol
ie — Intel 82586 Ethernet device driver, 7D-130
iee — EtherExpress 16 Ethernet device driver,

7D-133 ieef — Intel EtherExpress Flash32/82596 Ethernet device driver ieef and DLPI, 7D-136 ieef Primitives, 7D-137 ieef — Intel EtherExpress Flash32/82596 Ethernet device driver, 7D-136 if — general properties of Internet Protocol network interfaces, 7P-139 if_tcp — general properties of Internet Protocol network interfaces, 7P-139 inet — Internet protocol family

Intel 82586 Ethernet device driver — ie, 7D-130

Intel EtherExpress 16 Ethernet device driver — iee, 7D-133

Intel EtherExpress Flash32/82596 Ethernet device driver — ieef, 7D-136

Intel EtherExpress-Pro Ethernet device driver — eepro, 7D-89

Intel i82365SL PC Card Interface Controller — pcic, 7D-243

Internet Control Message Protocol — icmp

Internet Protocol — ip to Ethernet addresses — arp, 7P-17

Internet protocol family — inet

Internet Protocol network interfaces general properties — if_tcp, 7P-139

Internet Transmission Control Protocol — tcp

Internet User Datagram Protocol — udp ioctls for disks

   DKIOCEJECT — disk eject, 7I-78

   DKIOCGAPART — get full disk partition table,

7I-78

DKIOCGGEOM — get disk geometry, 7I-78

                                         ioctls for disks, continued

                                             DKIOCGVTOC — get volume table of contents

(vtoc), 7I-78

DKIOCINFO — get disk controller info, 7I-78

DKIOCSAPART — set disk partition info, 7I-78

DKIOCSGEOM — set disk geometry, 7I-78

DKIOCSVTOC — set volume table of contents

(vtoc), 7I-78 ioctls for floppy

FDEJECT — eject floppy, 7I-116

FDGETCHAGE — get status of disk changed,

7I-116

   FDIOCHAR — get floppy characteristics, 7I-116
ioctls for Internet socket descriptors

   SIOCSARP — set arp entry, 7P-17
ioctls for keyboards

   KIOCCMD — send a keyboard command,

7M-176

KIOCGCOMPAT — get compatibility mode,

7M-177

KIOCGDIRECT — get keyboard “direct input” state, 7M-177

KIOCGKEY — get translation table entry,

7M-176

KIOCGLED — get LEDs, 7M-177

KIOCGTRANS — get keyboard translation,

7M-175

KIOCLAYOUT — get keyboard type, 7M-176

KIOCSCOMPAT — set compatibility mode,

7M-177

KIOCSDIRECT — set keyboard “direct input” state, 7M-177

KIOCSKEY — change translation table entry,

7M-175

KIOCSLED — set LEDs, 7M-176

KIOCTRANS — set keyboard translation,

7M-175

   KIOCTYPE — get keyboard type, 7M-176
ioctls for sockets

   SIOCDARP — delete arp entry, 7P-17

   SIOCGARP — get arp entry, 7P-17
ioctl’s for terminals

   TIOCPKT — set/clear packet mode (pty),

7D-268

TIOCREMOTE — remote input editing, 7D-268
ioctl’s for terminals, continued

   TIOCSTART — start output (like control-Q),

7D-268

TIOCSTOP — stop output (like control-S),

7D-268 ip — Internet Protocol
ipd — STREAMS modules and drivers for the

Point-to-Point Protocol, 7M-260 ipdcm — STREAMS modules and drivers for the

Point-to-Point Protocol, 7M-260 ipdptp — STREAMS modules and drivers for the

Point-to-Point Protocol, 7M-260 ipi — IPI driver
ipi — IPI driver
isdnio — generic ISDN interface, 7I-151

ISO 9660 — ISO 9660 CD-ROM filesystem — hsfs,

7FS-125 isp — ISP SCSI Host Bus Adapter Driver, 7D-165

ISP SCSI Host Bus Adapter Driver — isp, 7D-165 iss — low-level module for Tricord System’s SCSI host bus adapter, 7D-169 K

kb — keyboard, 7M-171, 7M-177
kdmouse — built-in mouse device interface, 7D-178 kernel statistics driver — kstat, 7D-180 kernel symbols — ksyms, 7D-181 keyboard — system console keyboard, 7D-179 keyboard STREAMS module — kb, 7M-171

KIOCCMD — send a keyboard command, 7M-176

KIOCGCOMPAT — get compatibility mode, 7M-177

KIOCGDIRECT — get keyboard “direct input” state,

7M-177

KIOCGKEY — get translation table entry, 7M-176

KIOCGLED — get LEDs, 7M-177

KIOCGTRANS — get keyboard translation, 7M-175

KIOCLAYOUT — get keyboard type, 7M-176

KIOCSCOMPAT — set compatibility mode, 7M-177

KIOCSDIRECT — set keyboard “direct input” state,

7M-177

KIOCSKEY — change translation table entry, 7M-175

KIOCSLED — set LEDs, 7M-176

                                             KIOCTRANS — set keyboard translation, 7M-175

                                             KIOCTYPE — get keyboard type, 7M-176

                                             kstat — kernel statistics driver, 7D-180

                                             kyms — kernel symbols, 7D-181

L LAN support module — gld, 7D-120 ldterm — line discipline for STREAMS terminal module, 7M-183 le — Am7990 (LANCE) Ethernet device driver,

7D-186 lebuffer — Am7990 (LANCE) Ethernet device driver, 7D-186 ledma — Am7990 (LANCE) Ethernet device driver,

7D-186 leo — double-buffered 24-bit SBus color frame buffer and graphics accelerator, 7D-190 line discipline for unique stream connections

—connld, 7M-68 llc1 — Logical Link Control Protocol Class 1

Driver, 7D-191 log — interface to STREAMS error logging and event tracing, 7D-195 logi — LOGITECH bus mouse device interface,

7D-199

Logical Link Control Protocol Class 1 Driver — llc1, 7D-191

LOGITECH Bus Mouse device interface — logi,

7D-199 loopback file system — lofs, 7FS-194 loopback transport providers

— ticlts, 7D-369

— ticots, 7D-369

— ticotsord, 7D-369 low-level module

Adaptec 154x ISA host bus adapter — aha,

7D-14

Adaptec 174x EISA host bus adapter — eha,

7D-93

Dell SCSI Array Controller (DSA) — dsa,

7D-88

Mylex DAC960 and IBM DMC960 host bus adapter series — mlx, 7D-208 low-level module for Adaptec 7770 based SCSI controllers — esa, 7D-103 low-level module for Adaptec 7870 based SCSI controllers — adp, 7D-13 low-level module for Compaq SMART SCSI Array

Controller — csa, 7D-71 low-level module for NCR 53C710, 53C810, 53C815,

53C820, and 53C825 host bus adapters — ncrs, 7D-223 low-level module for the AMD PCscsi, PCscsi II, and PCnet-SCSI PCI-to-SCSI bus adapters — pcscsi, 7D-250 low-level module for Tricord System’s SCSI host bus adapter — iss, 7D-169 lp — driver for parallel port, 7D-200

M magnetic tape interface

— mtio, 7I-216 mcis — low-level module for IBM MicroChannel host bus adapter, 7D-202 mcpp — ALM-2 Parallel Printer port driver, 7D-203
mcpzsa — ALM-2 zilog 8530 SCC serial communications driver mem— image of core memory, 7D-207 memory based filesystem — tmpfs, 7FS-376 memory, core image — mem, 7D-207 memory, zeroed unnamed source — zero, 7D-412

Microsoft Bus Mouse device interface — msm,

7D-214 mlx — low-level module for Mylex DAC960 and

IBM DMC960 host bus adapter series, 7D-208

Board Configuration and Auto Configuration,

7D-208, 7D-210

EISA/Micro Channel Configuration Tips,

7D-208

Hot Plugging, 7D-213

SCSI Target IDs, 7D-213

Standby Drives, 7D-212 monitor

PROM monitor configuration interface —

openprom, monitor, continued

7D-235 monochrome frame buffer — bwtwo, 7D-52

Mouse device interface

LOGITECH Bus Mouse device interface —

          logi, 7D-199
msm — Microsoft Bus Mouse device interface,

7D-214 mtio — general magnetic tape interface, 7I-216

Mylex DAC960 and IBM DMC960 host bus adapter series low-level module — mlx, 7D-208 N

ncrs — low-level module for NCR 53C710, 53C810,

53C820, and 53C825 host bus adapters, 7D-223

NE2000, NE2000plus Ethernet device driver, Novell

— nei, 7D-228

NE3200 Ethernet device driver, Novell — nee,

7D-225 nei — NE3200 Ethernet device driver, 7D-225
nei — NE2000, NE2000plus Ethernet device driver,

7D-228

Netflex-2 Ethernet device driver, Compaq — nfe,

7D-231 nei — Netflex-2 Ethernet device driver, 7D-231

Novell NE2000, NE2000plus Ethernet device driver

— nei, 7D-228

Novell NE3200 Ethernet device driver — nee,

7D-225 null — null file, 7D-234

O

openprom — PROM monitor configuration interface, 7D-235 P parallel port, bi-directional — bpp, 7D-43 driver for parallel port — lp, 7D-200 pcelx — 3COM EtherLink III PCMCIA Ethernet

Adapter, 7D-239

PCFS — DOS formatted file system, 7FS-240
pcic — Intel i82365SL PC Card Interface Controller, 7D-243 pckt — STREAMS Packet Mode module, 7M-245

PCMCIA memory card nexus driver — pcmem,

7D-246

PCMCIA RAM memory card device driver — pcram, 7D-249

PCMCIA serial card device driver — pcser,

7D-251 pcmem — PCMCIA memory card nexus driver,

7D-246 pcn — AMD PCnet Ethernet controller device driver, 7D-247 pcram — PCMCIA RAM memory card device driver, 7D-249 pcscsi — low-level module for the AMD PCscsi,

PCscsi II, and PCnet-SCSI PCI-to-SCSI bus adapters, 7D-250 pcser — PCMCIA serial card device driver, 7D-251
pe — Xircom Pocket Ethernet device driver, 7D-252
pfmod — STREAMS packet filter module, 7M-255
pipemod — STREAMS pipe flushing module,

7M-258

Platform Specific Module (PSM) for Tricord Systems

Enterprise Server Models ES3000, ES4000 and

ES5000 — tpf, 7D-378 pln — SPARC Storage Array SCSI Host Bus adapter driver, 7D-259

PLN SCSI Host Bus Adapter driver — pln, 7D-259

Point-to-Point Protocol

— ipd, 7M-260

— ipdcm, 7M-260

— ipdptp, 7M-260

— ppp, 7M-260

— ppp_diag, 7M-260 ppp — STREAMS modules and drivers for the

Point-to-Point Protocol, 7M-260

Operation, 7M-260 ppp_diag — STREAMS modules and drivers for the Point-to-Point Protocol, 7M-260

PROM

PROM, continued monitor configuration interface — openprom,

7D-235

Pseudo Terminal Emulation module, STREAMS — ptem, 7M-262 pseudo-terminal driver — pty, 7D-267 ptem — STREAMS Pseudo Terminal Emulation module, 7M-262 ptm — STREAMS Buffer module, 7D-263
pts — STREAMS pseudo-tty slave driver, 7D-265
pty — pseudo-terminal driver, 7D-267
pty — pseudo-terminal driver

Q

qe — Am79C940 (MACE) Ethernet device driver
qec — Am79C940 (MACE) Ethernet device driver
quotactl() — disk quotas, 7I-274

R Racal Interlan ES-3210 Ethernet Adapter driver — riles, 7D-276 remote input editing ioctl — TIOCREMOTE,

7D-268 riles — device driver for the Racal Interlan ES-

3210 Ethernet Adapter, 7D-276 S

sbpro — Creative Labs Sound Blaster audio device

D"", 7D-283

SCSI disk devices driver — sd, 7D-285

SCSI tape devices driver — st, 7D-304 sd — driver for SCSI disk devices, 7D-285 send a keyboard command ioctl — KIOCCMD,

7M-176 serial communications driver — zs

Serial Optical Controller device driver — soc,

7D-299

Serial Parallel Communications driver for SBus — stc, 7D-314 set compatibility mode ioctl — KIOCSCOMPAT,

7M-177 set keyboard “direct input” state ioctl —

KIOCSDIRECT, 7M-177 set keyboard translation ioctl — KIOCTRANS,

7M-175 set LEDs ioctl — KIOCSLED, 7M-176 set/clear packet mode (pty) ioctl — TIOCPKT, 7D-268

SIOCDARP — delete arp entry, 7P-17

SIOCGARP — get arp entry, 7P-17

SIOCSARP — set arp entry, 7P-17

SMC 3032/EISA dual-channel Ethernet device driver — smce, 7D-292

SMC 8003/8013/8216/8416 Ethernet device driver

— smc, 7D-289 smc — SMC 8003/8013/8216/8416 Ethernet device driver, 7D-289

SMC Elite32 Ultra (8232) Ethernet device driver — smceu, 7D-295

SMC Ether100 (9232) Ethernet device driver — smcf, 7D-297

SMC EtherPower 8432BT Ethernet controller device driver — dnet, 7D-85 smce — SMC 3032/EISA dual-channel Ethernet device driver, 7D-292 smceu — SMC Elite32 Ultra (8232) Ethernet device driver, 7D-295 smcf — SMC Ether100 (9232) Ethernet device driver, 7D-297

SMD and IPI disk control operations — hdio,

7I-123

SMD disk controller

Xylogics 450 — xy

Xylogics 451 — xy

Xylogics 7053 — xd soc — Serial Optical Controller Device Driver,

7D-299 sockio — ioctls that operate directly on sockets,

7I-301 sockets ioctrls that operate directly — sockio, 7I-301

Solaris VISUAL I/O control operations, 7I-393

Sound Blaster 16 audio device — sbpro, 7D-283

Sound Blaster AWE32 audio device — sbpro,

7D-283

Sound Blaster Pro audio device — sbpro, 7D-283

SPARCstorage Array disk devices driver — ssd, 7D-302

SCSI Host Bus Adapter driver — pln, 7D-259 ssd — driver for SPARC Storage Array disk devices, 7D-302 st — driver for SCSI tape devices, 7D-304 start output (like control-Q) ioctl —

   TIOCSTART, 7D-268
stc — Serial Parallel Communications driver for

SBus, 7D-314 stop output (like control-S) ioctl — TIOCSTOP,

7D-268

STP 4020 PCMCIA Adapter

STP 4020 PCMCIA Adapter, 7D-325 stp4020 — STP 4020 PCMCIA Adapter, 7D-325

STREAMS console interface — console, 7D-69 interface to error logging — log, 7D-195 interface to event tracing — log, 7D-195 keyboard module — kb, 7M-171 line discipline for unique stream connections — connld, 7M-68 loopback transport providers — ticlts, ticots, ticotsord, 7D-369

On-board serial HDLC interface — zsh standard terminal line discipline module — ldterm, 7M-183

Transport Interface cooperating module — timod, 7M-371

Transport Interface read/write interface module — tirdwr, 7M-374

V7, 4BSD, XENIX compatibility module — ttcompat, 7M-384

STREAMS Administrative Driver — sad, 7D-280

STREAMS Buffer module — bufmod, 7M-48,

7D-263

STREAMS ioctl commands — streamio, 7I-326

STREAMS module

SunButtons and SunDials — bd, 7M-38

STREAMS modules and drivers for the Point-to-

Point Protocol

— ipd, 7M-260

— ipdcm, 7M-260

— ipdptp, 7M-260

— ppp, 7M-260

— ppp_diag, 7M-260

STREAMS Packet Filter Module — pfmod, 7M-255

STREAMS Packet Mode module — pckt, 7M-245

STREAMS pipe flushing module — pipemod,

7M-258

STREAMS Pseudo Terminal Emulation module — ptem, 7M-262

STREAMS pseudo-tty slave driver — pts, 7D-265

SunButtons and SunDials STREAMS module — bd,

7M-38 system console display — display, 7D-77 system console keyboard — keyboard, 7D-179 T tape drive, 1/2-inch xt — Xylogics 472 tape interface — mt, 7D-215 tape, magnetic interface

— mtio, 7I-216 tcp — Internet Transmission Control Protocol
tcx — Sun low-range graphics accelerator with color memory frame buffer, 7D-344 terminal emulation, ANSI — wscons terminal interface

— termio, 7I-346 terminal interface, extended

— termiox, 7I-364 terminal parameters — termiox, 7I-364 terminal, standard STREAMS line discipline module — ldterm, 7M-183 termio — general terminal interface, 7I-346
termiox — extended general terminal interface,

7I-364 ticlts — loopback transport provider, 7D-369
ticots — loopback transport provider, 7D-369
ticotsord — loopback transport provider, 7D-369
timod — Transport Interface cooperating module,

7M-371, 7M-374

TIOCPKT — set/clear packet mode (pty), 7D-268

TIOCREMOTE — remote input editing, 7D-268

TIOCSTART — start output (like control-Q), 7D-268

TIOCSTOP — stop output (like control-S), 7D-268
tiqmouse — integrated mouse interface, 7D-373
tmpfs — memory based filesystem, 7FS-376
tpf — Platform Specific Module (PSM) for Tricord

Systems Enterprise Server Models ES3000,

ES4000 and ES5000, 7D-378 tr — IBM 16/4 token ring network device driver,

7D-379

Transport Interface cooperating STREAMS module

— timod, 7M-371

Transport Interface read/write interface STREAMS module — timod, 7M-374 trantor — Trantor T348 Parallel SCSI host bus adapter, 7D-382

Trantor T348 Parallel SCSI host bus adapter —

   trantor, 7D-382
ttcompat — V7, 4BSD and XENIX STREAMS compatibility module, 7M-384 tty — controlling terminal interface, 7D-390

U

udp — Internet User Datagram Protocol unnamed zeroed memory source — zero, 7D-412 V V7 compatibility module — ttcompat, 7M-384 volfs — Volume Management file system, 7FS-395

Volume Management file system — volfs, 7FS-395 vuid2ps2 — converts mouse protocol to Firm

Events, 7M-397 vuid3ps2 — converts mouse protocol to Firm

Events, 7M-397 vuidm3p — converts mouse protocol to Firm

Events, 7M-397 vuidm4p — converts mouse protocol to Firm

Events, 7M-397 vuidm5p — converts mouse protocol to Firm

Events, 7M-397 vuidmice — converts mouse protocol to Firm

Events, 7M-397 W workstation console — wscons, 7D-399 X

xd — Xylogics SMD Disk driver

XENIX compatibility module — ttcompat,

7M-384 xt — Xylogics 472 1/2-inch tape drive
xy — Xylogics SMD Disk driver

Xylogics 472 1/2-inch tape drive — xt

Xylogics SMD Disk driver — xd, 7D-406 thru

7D-411 Z

zero — source of zeroes, 7D-412

Zilog 8530 SCC serial communications driver — zs zs — zilog 8530 SCC serial communications driver
zsh — On-board serial HDLC interface