SunOS 5.5 Kernel Functions for Drivers makecom (9F)

NAME makecom, makecom_g0, makecom_g0_s, makecom_g1, makecom_g5 − make a packet for

SCSI commands

SYNOPSIS #include <sys/scsi/scsi.h> void makecom_g0(struct scsi_pkt ∗pkt, struct scsi_device ∗devp, int flag, int cmd, int addr, int cnt);

void makecom_g0_s(struct scsi_pkt ∗pkt, struct scsi_device ∗devp, int flag, int cmd, int cnt, int fixbit);

void makecom_g1(struct scsi_pkt ∗pkt, struct scsi_device ∗devp, int flag, int cmd, int addr, int cnt);

void makecom_g5(struct scsi_pkt ∗pkt, struct scsi_device ∗devp, int flag, int cmd, int addr, int cnt);

INTERFACE

LEVEL Solaris DDI specific (Solaris DDI).

ARGUMENTS pkt Pointer to an allocated scsi_pkt (9S) structure.

devp Pointer to the target’s scsi_device (9S) structure.

flag Flags for the pkt_flags member.

cmd First byte of a group 0 or 1 or 5 SCSI CDB.

addr Pointer to the location of the data.

cnt Number of bytes to transfer.

fixbit Fixed bit in sequential access device commands.

DESCRIPTION makecom functions initialize a packet with the specified command descriptor block, devp and transport flags. The pkt_address , pkt_flags , and the command descriptor block pointed to by pkt_cdbp are initialized using the remaining arguments. Target drivers may use makecom_g0( ) for Group 0 commands (except for sequential access devices), or makecom_g0_s( ) for Group 0 commands for sequential access devices, or makecom_g1( ) for Group 1 commands, or makecom_g5( ) for Group 5 commands. fixbit is used by sequential access devices for accessing fixed block sizes and sets the the tag portion of the

SCSI CDB.

CONTEXT These functions can be called from user or interrupt context.

EXAMPLE if (blkno >= (1<<20)) { makecom_g1(pkt, SD_SCSI_DEVP, pflag, SCMD_WRITE_G1,

(int) blkno, nblk);

}else { makecom_g0(pkt, SD_SCSI_DEVP, pflag, SCMD_WRITE,

(int) blkno, nblk); } modified 30 Aug 1995 9F-265 makecom (9F) Kernel Functions for Drivers SunOS 5.5

SEE ALSO scsi_device (9S), scsi_pkt (9S)

ANSI Small Computer System Interface-2 (SCSI-2)

WritingDevice Drivers

9F-266 modified 30 Aug 1995