SunOS 5.5 Data Structures for Drivers datab (9S)

NAME datab − STREAMS message data structure

SYNOPSIS #include <sys/stream.h>

INTERFACE

LEVEL Architecture independent level 1 (DDI/DKI).

DESCRIPTION The datab structure describes the data of a STREAMS message. The actual data contained in a STREAMS message is stored in a data buffer pointed to by this structure. A msgb (message block) structure includes a field that points to a datab structure.

A data block can have more than one message block pointing to it at one time, so the db_ref member keeps track of a data block’s references, preventing it from being deallocated until all message blocks are finished with it.

STRUCTURE

MEMBERS unsigned char ∗db_base; /∗ first byte of buffer ∗/ unsigned char ∗db_lim; /∗ last byte (+1) of buffer ∗/ unsigned char db_ref; /∗ # of message pointers to this data ∗/ unsigned char db_type; /∗ message type ∗/

A datab structure is defined as type dblk_t .

SEE ALSO free_rtn (9S), msgb(9S)

WritingDevice Drivers

STREAMSProgramming Guide modified 11 Apr 1991 9S-17