SunOS 5.5 Data Structures for Drivers kstat_named (9S)

NAME kstat_named − structure for named kstats

SYNOPSIS #include <sys/types.h>

#include <sys/kstat.h>

#include <sys/ddi.h>

#include <sys/sunddi.h>

INTERFACE

LEVEL Solaris DDI specific (Solaris DDI)

DESCRIPTION Named kstats are an array of name-value pairs. These pairs are kept in the kstat_named structure. When a kstat is created by kstat_create (9F), the driver specifies how many of these structures will be allocated. They are returned as an array pointed to by the ks_data field.

STRUCTURE

MEMBERS union { char c[16];

long l;

ulong_t ul;

longlong_t ll;

u_longlong_t ull;

}value; /∗ value of counter ∗/

The only member exposed to drivers is the value member. This field is a union of several data types. The driver must specify which type it will use in the call to kstat_named_init( ).

SEE ALSO kstat_create (9F), kstat_named_init (9F)

WritingDevice Drivers modified 4 Apr 1994 9S-49