ddi_idevice_cookie (9S) Data Structures for Drivers SunOS 5.5

NAME ddi_idevice_cookie − device interrupt cookie

SYNOPSIS #include <sys/ddi.h>

#include <sys/sunddi.h>

INTERFACE

LEVEL Solaris DDI specific (Solaris DDI).

DESCRIPTION The ddi_idevice_cookie_t structure contains interrupt priority and interrupt vector information for a device. This structure is useful for devices having programmable businterrupt levels. ddi_add_intr (9F) assigns values to the ddi_idevice_cookie_t structure members.

STRUCTURE

MEMBERS u_short idev_vector; / ∗ interrupt vector ∗/ u_short idev_priority; / ∗ interrupt priority ∗/

The idev_vector field contains the interrupt vector number for vectored bus architectures such as VMEbus. The idev_priority field contains the bus interrupt priority level.

SEE ALSO vme (4), ddi_add_intr (9F)

WritingDevice Drivers

9S-38 modified 13 Sep 1994