#*******************************************************************************
#
# NAME:         default.def
# SUMMARY:      Default NVSRAM settings definition file for Solaris
# COMPONENT:    sonoma
# VERSION:      %rm6_1%
# UPDATE DATE:  %date_modified: Fri Sep 19 06:13:55 1997 %
# PROGRAMMER:   %created_by: bmyers %
#
#               Copyright 1997 by Symbios Logic Inc.
#
# DESCRIPTION:
#  This file contains default NVSRAM settings needed to operate the Solaris
#  rm6 applications when connected to Series 3 controllers. This file will be
#  used whenever nvutil is executed with the -v option and a filename is not
#  specified by the -n option. Additions to this file must include the following
#  information:
#
#       nvsramOffset - NVSRAM User Configuration byte offset in hex.
#       nvsramBitMask - Bit mask defining the bit to be verified.
#       nvsramValue - Value NVSRAM byte and defined bit(s) should be set to.
#       comments - Text entry description of defined NVSRAM byte and bit(s).
#
#  The following example specifies the format that must be used:
#
#  nvsramOffset    nvsramBitMask    nvsramValue        comments
#  0x8             0x10             0x10           Enable page 2B LUN number bit
#  0x11            0xff             0x00           Inquiry non-owned LUN
#
# NOTES:
#
#
# REFERENCE:
# 1.  PIP0003A.DOC, Source Code Integrity Measures
#
#
# CODING STANDARD WAIVERS:
#
#
#*******************************************************************************
#nvsramOffset   nvsramBitMask   nvsramValue             Comments
0x00		0x01		0x01		Enable Synchronous Negotiation
0x01		0x01		0x01		Enable Wide Negotiation
0x08		0x10		0x10		Enable page 2B LUN number bit
0x09		0x40		0x40		Enable > 2GB LUNs bit
0x0c		0x01		0x01		Download Response
0x11		0xff		0x20		Unconfigured LUNs bit
0x1c		0x40		0x00		Controller Quiesced Response
0x1d		0x40		0x00		AEN notification bit
0x1d		0x80		0x00		Status notification bit
0x24		0xff		0x00		Inquiry non-owned LUN
0x28		0x80		0x00		Create default LUN
0x28		0x04		0x04		Enable synchronization bit
0x29            0x08            0x08            Enable reserve/release on alt ctl
0x2d		0xff		0x00		Battery Expiration Age
0x2e		0xff		0x00		Battery Expiration Warning
0x2F		0x80		0x80		Enable WWN in Standard Inquiry
