enable (1) User Commands SunOS 5.5

NAME enable, disable − enable/disable LP printers

SYNOPSIS /usr/bin/enable printer ...

/usr/bin/disable [ − c | − W ] [ − r [ reason ]] printer ...

AVAILABILITY SUNWlpu

DESCRIPTION The enable command activates the named printer s, enabling them to print requests submitted by the lp command. If the printer is remote, the command will only enable the transfer of requests to the remote system; the enable command must be run again, on the remote system, to activate the printer. (Run lpstat − p to get the status of printer s.)

The disable command deactivates the named printer, disabling it from printing requests submitted by lp. By default, any requests that are currently printing on the designated printer(s) will be reprinted in their entirety either on the same printer or on another member of the same class of printers. If the printer is remote, this command will only stop the transmission of jobs to the remote system. The disable command must be run on the remote system to disable the printer. (Run lpstat − p to get the status of printer s.)

OPTIONS Options for use with disable are:

− c Cancel any requests that are currently printing on the designated printer(s).

This option cannot be used with the − W option. If the printer is remote, the

− c option will be silently ignored.

− W Wait until the request currently being printed is finished before disabling the specified printer. This option cannot be used with the − c option. If the printer is remote, the − W option will be silently ignored.

− r reason Assign a reason for the disabling of the printer(s). This reason applies to all printer s specified. This reason is reported by lpstat − p. reason must be enclosed in quotes if it contains blanks. The default reason is unknown reason for the existing printer, and new printer for a printer just added to the system but not yet enabled.

FILES /var/spool/lp/ ∗

SEE ALSO lp(1), lpstat (1)

1-254 modified 14 Sep 1992