SunOS 5.5 User Commands machid (1)

NAME machid, sun, iAPX286, i286, i386, i486, i860, pdp11, sparc, u3b, u3b2, u3b5, u3b15, vax, u370 − get processor type truth value

SYNOPSIS sun iAPX286 i386 pdp11 sparc u3b u3b2 u3b5 u3b15 vax u370

DESCRIPTION The following commands will return a true value (exit code of 0) if you are using an instruction set that the command name indicates.

sun True if you are on a Sun system.

iAPX286 True if you are on a computer using an iAPX286 processor.

i386 True if you are on a computer using an iAPX386 processor.

pdp11 True if you are on a PDP-11/45 ™ or PDP-11/70 ™ .

sparc True if you are on a computer using a SPARC-family processor.

u3b True if you are on a 3B20computer.

u3b2 True if you are on a 3B2computer.

u3b5 True if you are on a 3B5computer.

u3b15 True if you are on a 3B15computer.

vax True if you are on a VAX-11/750 ™ or VAX-11/780 ™ .

u370 True if you are on an IBM® System/370 ™ computer.

The commands that do not apply will return a false (non-zero) value. These commands are often used within makefiles (see make(1S)) and shell scripts (see sh(1)) to increase portability.

SEE ALSO make(1S), sh(1), test (1), true (1), uname (1)

NOTES The machid family of commands is obsolete. Use uname − p and uname − m instead.

modified 5 Jul 1990 1-567