SunOS 5.5 User Commands tplot (1)

NAME tplot, t300, t300s, t4014, t450, tek, ver − graphics filters for various plotters

SYNOPSIS /usr/bin/tplot [ − Tterminal ]

AVAILABILITY SUNWcsu

DESCRIPTION tplot reads plotting instructions from the standard input and produces plotting instructions suitable for a particular terminal on the standard output.

If no terminal is specified, the environment variable TERM is used. The default terminal is tek .

ENVIRONMENT Except for ver, the following terminal-types can be used with ‘lpr − g’(see lpr ) to produce plotted output:

300 DASI 300 or GSI terminal (Diablo® mechanism).

300s | 300S DASI 300s terminal (Diablo mechanism).

450 DASI Hyterm 450 terminal (Diablo mechanism).

4014 | tek Tektronix 4014 and 4015 storage scope with Enhanced Graphics Module.

(Use 4013 for Tektronix 4014 or 4015 without the Enhanced Graphics

Module).

ver Versatec ® D1200A printer-plotter. The output is scan-converted and suitable input to ‘lpr − v’.

FILES /usr/lib/t300

/usr/lib/t300s

/usr/lib/t4014

/usr/lib/t450

/usr/lib/tek

/usr/lib/vplot

SEE ALSO lp(1), vi(1) modified 14 Jul 1994 1-1085