SunOS 5.5 Miscellaneous Library Functions curs_insstr (3X)

NAME curs_insstr, insstr, insnstr, winsstr, winsnstr, mvinsstr, mvinsnstr, mvwinsstr, mvwinsnstr − insert string before character under the cursor in a curses window

SYNOPSIS cc [ flag ... ] file ... − lcurses [ library .. ]

#include <curses.h> int insstr(char ∗str);

int insnstr(char ∗str, int n);

int winsstr( WINDOW ∗win, char ∗str);

int winsnstr( WINDOW ∗win, char ∗str, int n);

int mvinsstr(int y, int x, char ∗str);

int mvinsnstr(int y, int x, char ∗str, int n);

int mvwinsstr( WINDOW ∗win, int y, int x, char ∗str);

int mvwinsnstr( WINDOW ∗win, int y, int x, char ∗str, int n);

MT-LEVEL Unsafe

DESCRIPTION With these routines, a character string (as many characters as will fit on the line) is inserted before the character under the cursor. All characters to the right of the cursor are moved to the right, with the possibility of the rightmost characters on the line being lost. The cursor position does not change (after moving to y, x, if specified). (This does not imply use of the hardware insert character feature.) The four routines with n as the last argument insert at most n characters. If n<=0, then the entire string is inserted.

If a character in str is a tab, newline, carriage return or backspace, the cursor is moved appropriately within the window. A newline also does a clrtoeol( ) before moving. Tabs are considered to be at every eighth column. If a character in str is another control character, it is drawn in the ^X notation. Calling winch( ) after adding a control character

(and moving to it, if necessary) does not return the control character, but instead returns the representation of the control character.

RETURN VALUES All routines return the integer ERR upon failure and an integer value other than ERR upon successful completion.

SEE ALSO curs_clear (3X),curs_inch (3X),curses (3X)

NOTES The header <curses.h> automatically includes the headers <stdio.h> and <unctrl.h> .

Note that all but winsnstr( ) may be macros.

modified 22 Jan 1993 3X-251