makedev (3C ) C Library Functions SunOS 5.5

NAME makedev, major, minor − manage a device number

SYNOPSIS #include <sys/types.h>

#include <sys/mkdev.h> dev_t makedev(major_t maj, minor_t min);

major_t major(dev_t device);

minor_t minor(dev_t device);

MT-LEVEL MT-Safe

DESCRIPTION The makedev( ) routine returns a formatted device number on success and NODEV on failure. maj is the major number. min is the minor number. makedev( ) can be used to create a device number for input to mknod (2).

The major( ) routine returns the major number component from device.

The minor( ) routine returns the minor number component from device.

RETURN VALUES On failure, NODEV is returned and errno is set to indicate the error.

ERRORS makedev( ) will fail if one or more of the following are true:

EINVAL One or both of the arguments maj and min is too large.

EINVAL The devicenumber created from maj and min is NODEV.

major( ) will fail if one or more of the following are true:

EINVAL The deviceargument is NODEV.

EINVAL The major number component of deviceis too large.

minor( ) will fail if the following is true:

EINVAL The deviceargument is NODEV.

SEE ALSO mknod (2), stat (2)

3C-662 modified 22 Jan 1993