SunOS 5.5 Kernel Functions for Drivers bp_mapin (9F)

NAME bp_mapin − allocate virtual address space

SYNOPSIS #include <sys/types.h>

#include <sys/buf.h> void bp_mapin(struct buf ∗bp);

INTERFACE

LEVEL Architecture independent level 1 (DDI/DKI).

ARGUMENTS bp Pointer to the buffer header structure.

DESCRIPTION bp_mapin( ) is used to map virtual address space to a page list maintained by the buffer header during a paged- I/O request. bp_mapin( ) allocates system virtual address space, maps that space to the page list, and returns the starting address of the space in the bp-

>b_un.b_addr field of the buf (9S) structure. Virtual address space is then deallocated using the bp_mapout (9F) function.

If a null page list is encountered, bp_mapin( ) returns without allocating space and no mapping is performed.

CONTEXT bp_mapin( ) can be called from user context only.

SEE ALSO bp_mapout (9F), buf (9S)

WritingDevice Drivers modified 13 Sep 1992 9F-51