SunOS 5.5 Kernel Functions for Drivers ddi_dma_free (9F)

NAME ddi_dma_free − release system DMA resources

SYNOPSIS #include <sys/ddi.h>

#include <sys/sunddi.h> int ddi_dma_free(ddi_dma_handle_t handle);

INTERFACE

LEVEL Solaris DDI specific (Solaris DDI).

ARGUMENTS handle The handle filled in by a call to ddi_dma_setup (9F).

DESCRIPTION ddi_dma_free( ) releases system DMA resources set up by ddi_dma_setup (9F). When a

DMA transfer completes, the driver should free up system DMA resources established by a call to ddi_dma_setup (9F). This is done by a call to ddi_dma_free( ). ddi_dma_free( ) does an implicit ddi_dma_sync (9F) for you so any further synchronization steps are not necessary.

RETURN VALUES ddi_dma_free( ) returns:

DDI_SUCCESS Successfully released resources

DDI_FAILURE Failed to free resources

CONTEXT ddi_dma_free( ) can be called from user or interrupt context.

SEE ALSO ddi_dma_addr_setup (9F), ddi_dma_buf_setup (9F), ddi_dma_htoc (9F), ddi_dma_sync (9F), ddi_dma_req (9S)

WritingDevice Drivers modified 13 Sep 1992 9F-121