ddi_report_dev (9F) Kernel Functions for Drivers SunOS 5.5

NAME ddi_report_dev − announce a device

SYNOPSIS #include <sys/conf.h>

#include <sys/ddi.h>

#include <sys/sunddi.h> void ddi_report_dev(dev_info_t ∗dip);

INTERFACE

LEVEL Solaris DDI specific (Solaris DDI).

ARGUMENTS dip a pointer the device’s dev_info structure.

DESCRIPTION ddi_report_dev( ) prints a banner at boot time, announcing the device pointed to by dip.

The banner is always placed in the system logfile (displayed by dmesg(1M)), but is only displayed on the console if the system was booted with the verbose (− v) argument.

CONTEXT ddi_report_dev( ) can be called from user or interrupt context.

SEE ALSO dmesg(1M), kernel (1M)

WritingDevice Drivers

9F-210 modified 7 Jun 1993