nulldev (9F) Kernel Functions for Drivers SunOS 5.5

NAME nulldev − zero return function

SYNOPSIS #include <sys/conf.h>

#include <sys/ddi.h> int nulldev( );

INTERFACE

LEVEL Architecture independent level 1 (DDI/DKI).

DESCRIPTION nulldev () returns 0. It is intended to be used in the cb_ops (9S) data structure of a device driver for device entry points that do nothing.

RETURN VALUES nulldev () returns a 0.

CONTEXT nulldev () can be called from any context.

SEE ALSO nodev (9F), cb_ops (9S)

WritingDevice Drivers

9F-280 modified 11 Apr 1991