rmalloc_wait (9F) Kernel Functions for Drivers SunOS 5.5

NAME rmalloc_wait − allocate space from a resource map, wait if necessary

SYNOPSIS #include <sys/map.h>

#include <sys/ddi.h> unsigned long rmalloc_wait(struct map ∗mp, size_t size);

INTERFACE

LEVEL Architecture independent level 1 (DDI/DKI).

ARGUMENTS mp Pointer to the resource map from which space is to be allocated.

size Number of units of space to allocate.

DESCRIPTION rmalloc_wait( ) requests an allocation of space from a resource map. rmalloc_wait( ) is similar to the rmalloc (9F) function with the exception that it will wait for space to become available if necessary.

RETURN VALUES rmalloc_wait( ) returns the base of the allocated space.

CONTEXT This functions can be called from user or interrupt context. However in most cases rmalloc_wait( ) should be called from user context only.

SEE ALSO rmalloc (9F), rmallocmap (9F), rmfree (9F), rmfreemap (9F)

WritingDevice Drivers

9F-318 modified 28 Apr 1992