scsi_log (9F) Kernel Functions for Drivers SunOS 5.5

NAME scsi_log − display a SCSI-device-related message

SYNOPSIS #include <sys/scsi/scsi.h> #include <sys/cmn_err.h> void scsi_log(dev_info_t ∗dip, char ∗drv_name, u_int level, const char ∗fmt, ...);

INTERFACE

LEVEL Solaris DDI specific (Solaris DDI).

ARGUMENTS dip Pointer to the dev_info structure.

drv_name String naming the device.

level Error level.

fmt Display format.

DESCRIPTION scsi_log( ) is a utility function that displays a message via the cmn_err (9F) routine. The error levels that can be passed in to this function are CE_PANIC, CE_WARN, CE_NOTE,

CE_CONT, and SCSI_DEBUG. The last level is used to assist in displaying debug messages to the console only. drv_name is the short name by which this device is known; example disk driver names are sd and cmdk . If the dev_info_t pointer is NULL, then the drv_name will be used with no unit or long name.

EXAMPLE scsi_log(dev, "Disk Unit ", CE_PANIC, "Bad Value %d\n", foo);

Generates:

PANIC: /eisa/aha@330,0/cmdk@0,0 (Disk Unit 0): Bad Value 5

Followed by a PANIC.

scsi_log(dev, "sd", CE_WARN, "Label Bad\n");

Generates:

WARNING: /sbus@1,f8000000/esp@0,8000000/sd@1,0 (sd1): Label Bad scsi_log((dev_info_t ∗) NULL, "Disk Unit ", CE_NOTE, "Disk Ejected\n");

Generates:

Disk Unit : Disk Ejected scsi_log(cmdk_unit, "Disk Unit ", CE_CONT, "Disk Inserted\n");

Generates:

Disk Inserted scsi_log(sd_unit, "sd", SCSI_DEBUG, "We really got here\n");

Generates (only to the console):

DEBUG: sd1: We really got here

CONTEXT scsi_log( ) may be called from user or interrupt context.

9F-354 modified 7 Jun 1993

SunOS 5.5 Kernel Functions for Drivers scsi_log (9F)

SEE ALSO cmn_err (9F), scsi_errmsg (9F)

WritingDevice Drivers modified 7 Jun 1993 9F-355