qunbufcall (9F) Kernel Functions for Drivers SunOS 5.5

NAME qunbufcall − cancel a pending qbufcall request

SYNOPSIS #include <sys/stream.h>

#include <sys/ddi.h> void qunbufcall(queue_t ∗q, int id);

INTERFACE

LEVEL Solaris DDI specific (Solaris DDI).

ARGUMENTS q Pointer to STREAMS queue_t structure.

id Identifier returned from qbufcall (9F)

DESCRIPTION qunbufcall cancels a pending qbufcall( ) request. The argument id is a non-zero identifier of the request to be cancelled. id is returned from the qbufcall( ) function used to issue the cancel request.

The qunbufcall( ) function is tailored to be used with the enhanced STREAMS framework interface which is based on the concept of perimeters. (See mt-streams (9F) man page.) qunbufcall( ) returns when the bufcall has been cancelled or finished executing.

The bufcall will be cancelled even if it is blocked at the perimeters associated with the queue. All outstanding bufcalls should be cancelled before the driver closes or module returns.

CONTEXT qunbufcall( ) can be called from user or interrupt context.

SEE ALSO mt-streams (9F), qbufcall (9F), qtimeout (9F), quntimeout (9F)

WritingDevice Drivers

STREAMSProgramming Guide

9F-310 modified 10 Jan 1993