unbufcall (9F) Kernel Functions for Drivers SunOS 5.5

NAME unbufcall − cancel a pending bufcall request

SYNOPSIS #include <sys/stream.h> void unbufcall(int id);

INTERFACE

LEVEL Architecture independent level 1 (DDI/DKI).

ARGUMENTS id Identifier returned from bufcall (9F) or esbbcall (9F)

DESCRIPTION unbufcall cancels a pending bufcall( ) or esbbcall( ) request. The argument id is a nonzero identifier for the request to be cancelled. id is returned from the bufcall( ) or esbbcall( ) function used to issue the request.

unbufcall( ) will not return until the pending callback is cancelled or has run. Because of this, locks acquired by the callback routine should not be held across the call to unbufcall( ) or deadlock may result.

RETURN VALUES None.

CONTEXT unbufcall( ) can be called from user or interrupt context.

SEE ALSO bufcall (9F), esbbcall (9F)

WritingDevice Drivers

STREAMSProgramming Guide

9F-386 modified 19 Nov 1992