SunOS 5.5 Kernel Functions for Drivers ddi_prop_get_int (9F)

NAME ddi_prop_get_int − lookup integer property

SYNOPSIS #include <sys/ddi.h>

#include <sys/sunddi.h> int ddi_prop_get_int(dev_t match_dev, dev_info_t ∗dip, u_int flags, char ∗name, int defvalue);

ARGUMENTS match_dev Device number associated with property or DDI_DEV_T_ANY.

dip Pointer to the device info node of device whose property list should be searched.

flags Possible flag values are some combination of:

DDI_PROP_DONTPASS

Do not pass request to parent device information node if property not found.

DDI_PROP_NOTPROM

Do not look at PROM properties (ignored on platforms that do not support PROM properties).

name String containing the name of the property.

defvalue An integer value that is returned if the property cannot be found.

INTERFACE

LEVEL Solaris DDI specific (Solaris DDI).

DESCRIPTION ddi_prop_get_int( ) searches for an integer property and, if found, returns the value of the property.

Properties are searched for based on the dip, name, match_dev, and the type of the data

(integer). The property search order is as follows:

1. Search software properties created by the driver.

2. Search the software properties created by the system (or nexus nodes in the device info tree).

3. Search the driver global properties list.

4. If DDI_PROP_NOTPROM is not set, search the PROM properties (if they exist).

5. If DDI_PROP_DONTPASS is not set, pass this request to the parent device information node.

6. Return DDI_PROP_NOT_FOUND.

Usually, the match_dev argument should be set to the actual device number that this property is associated with. However, if the match_dev argument is DDI_DEV_T_ANY, then ddi_prop_get_int( ) will match the request regardless of the match_dev the property was created with. If a property was created with match_dev set to DDI_DEV_T_NONE, then the only way to look up this property is with a match_dev set to DDI_DEV_T_ANY. PROM properties are always created with match_dev set to DDI_DEV_T_NONE.

modified 17 Nov 1994 9F-189 ddi_prop_get_int (9F) Kernel Functions for Drivers SunOS 5.5 name must always be set to the name of the property being looked up.

The return value of the routine is the value of the property. If the property is not found, the argument defvalueis returned as the value of the property.

RETURN VALUES ddi_prop_get_int( ) returns the value of the property. If the property is not found, the argument defvalueis returned.

CONTEXT ddi_prop_get_int( ) can be called from user or kernel context.

EXAMPLES The following example demonstrates the use of ddi_prop_get_int( ). /∗ ∗ Get the value of the integer "width" property, using

∗ our own default if no such property exists ∗/ width = ddi_prop_get_int(xx_dev, xx_dip, 0, "width",

XX_DEFAULT_WIDTH);

SEE ALSO ddi_prop_exists (9F), ddi_prop_lookup(9F), ddi_prop_update (9F), ddi_prop_remove (9F)

WritingDevice Drivers

9F-190 modified 17 Nov 1994