SunOS 5.5 Maintenance Commands prtvtoc (1M )

NAME prtvtoc − report information about a disk geometry and partitioning

SYNOPSIS prtvtoc [ − fhs ] [ − t vfstab ] [ − m mnttab ] device

AVAILABILITY SUNWcsu

DESCRIPTION The prtvtoc command allows the contents of the VTOC (volume table of contents) to be viewed. The command can be used only by the super-user.

The devicename can be the file name of a raw device in the form of /dev/rdsk/c?t?d?s2 or can be the file name of a block device in the form of /dev/dsk/c?t?d?s2 .

OPTIONS The following options are supported:

− f Report on the disk free space, including the starting block address of the free space, number of blocks, and unused partitions.

− h Omit the headers from the normal output.

− s Omit all headers but the column header from the normal output.

− t vfstab Use vfstab as the list of filesystem defaults, in place of /etc/vfstab .

− m mnttab Use mnttab as the list of mounted filesystems, in place of /etc/mnttab .

EXAMPLES The command line entry and system response shown below are for a 424-megabyte hard disk:

example# prtvtoc /dev/rdsk/c0t3d0s2

∗ /dev/rdsk/c0t3d0s2 partition map ∗ ∗ Dimension:

∗ 512 bytes/sector

∗ 80 sectors/track

∗ 9 tracks/cylinder

∗ 720 sectors/cylinder

∗ 2500 cylinders

∗ 1151 accessible cylinders ∗ ∗ Flags:

∗ 1: unmountable

∗ 10: read-only ∗ modified 25 Aug 1995 1M-497 prtvtoc (1M ) Maintenance Commands SunOS 5.5

∗ First Sector Last

∗ Partition Tag Flags Sector Count Sector Mount Directory

0 2 00 0 76320 76319 /

1 3 01 76320 132480 208799

2 5 00 0 828720 828719

5 6 00 208800 131760 340559 /opt

6 4 00 340560 447120 787679 /usr

7 8 00 787680 41040 828719 /export/home example#

Codes for TAG are:

NAME NUMBER

UNASSIGNED 0

BOOT 1

ROOT 2

SWAP 3

USR 4

BACKUP 5

VAR 7

HOME 8

FLAG indicates how the partition is to be mounted.

NAME NUMBER

MOUNTABLE, READ AND WRITE 00

NOT MOUNTABLE 01

MOUNTABLE, READ ONLY 10

The following example shows output for the − f option for the same disk as above.

example# prtvtoc − f /dev/rdsk/c0t3d0s0

FREE_START=0 FREE_SIZE=0 FREE_COUNT=0 FREE_PART=4 example#

SEE ALSO devinfo (1M), fmthard (1M), format (1M)

WARNINGS The mount command does not check the "not mountable" bit.

1M-498 modified 25 Aug 1995