SunOS 5.5 Maintenance Commands re-preinstall (1M )

NAME re-preinstall − installs the JumpStart software on a system

SYNOPSIS cdrom-mnt-pt /export/exec/ arch.release/sbin/install.d/re-preinstall

[ − m cdrom-mnt-pt ] [ − k platform_name ] target-slice

AVAILABILITY SUNWcdrom (Solaris CD).

DESCRIPTION re-preinstall installs the JumpStart software (Preinstall Boot Image) on a system, so you can power-on the system and have it automatically install the Solaris software (perform a

JumpStart installation on the system). Some new systems have the JumpStart software already preinstalled.

There are two ways to use the re-preinstall command. The most common way is to run re-preinstall on a system to install the JumpStart software on its own default boot disk.

This is useful if you want to restore a system to its original factory conditions.

You can also run re-preinstall on a system to install JumpStart software on any attached disk. Once you install the JumpStart software on a disk, you can move the disk to a different system and perform a JumpStart installation on the different system.

NOTE: While the command is valid for x86 systems, it is not useful because you cannot reboot with arguments.

re-preinstall creates a standard file system on the specified target-slice (usually slice 0), and re-preinstall makes sure there is enough space on the target-slice for the JumpStart software, which usually requires 26 Mbytes. If sufficient space is not available, repreinstall fails with the following message:

re-preinstall: target-slice is less than 26 Megabytes, please reformat it.

You can use the format (1M) command to create sufficient space on the target-slice for the

JumpStart software.

OPTIONS The following options are supported:

− m cdrom-mnt-pt Absolute path, or mount point, to the Solaris CD. The default is

/cdrom .

− k platform_name Platform name of the system that will use the disk with the

JumpStart software. The default is the platform name of the system running re-preinstall . (Use the uname − i command to determine a system’s platform name.)

OPERANDS The following operand is supported:

target-slice Device name of the disk slice where the JumpStart software will be installed (usually slice 0). For example, c0t3d0s0 .

EXAMPLES re-preinstall on a system and install the JumpStart software on its own default boot disk:

1. Boot the system from the Solaris CD in single-user mode at the "ok" prompt.

ok boot cdrom -s modified 13 Jan 1995 1M-513 re-preinstall (1M ) Maintenance Commands SunOS 5.5

2. When the system is in single-user mode, use the eeprom (1M) command to determine the system’s default boot disk. If no slice is specified for the system’s default boot disk, the system boots from slice 0 of the specified disk, by default.

Note that when you turn on a re-preinstalled system, the system looks for the JumpStart software on the disk slice that it boots from.

3. Run the re-preinstall command with only the target-slice argument; target-slice must be the device name of the disk you determined in Step 2.

For example, the following command installs the JumpStart software on the system’s default boot disk, c0t3d0s0 :

example# /cdrom/export/exec/sparc.Solaris_2.4/sbin/install.d/re-preinstall\ c0t3d0s0

EXIT STATUS The following exit values are returned:

0 success

1 an error has occurred.

SEE ALSO uname (1), format (1M), eeprom (1M), mount(1M)

SPARC:Installing Solaris Software

1M-514 modified 13 Jan 1995