rem_drv (1M ) Maintenance Commands SunOS 5.5

NAME rem_drv − remove a device driver from the system

SYNOPSIS rem_drv [ − b basedir ] device_driver

AVAILABILITY SUNWcsu

DESCRIPTION The rem_drv command informs the system that the device driver device_driveris no longer valid. If possible, rem_drv unloads device_driverfrom memory. Entries for the device in the /devices namespace are removed. rem_drv also updates the system driver configuration files.

If rem_drv has been executed, the next time the system is rebooted it will automatically perform a reconfiguration boot (see kernel (1M)).

OPTIONS − b basedir Sets the path to the root directory of the diskless client. Used on the server to execute rem_drv for a client. The client machine must be rebooted to unload the driver.

EXAMPLES The following example removes the sd driver from use:

example% rem_drv sd

The next example removes the driver from the sun1 diskless client. The driver will not be uninstalled nor unloaded until the client machine is rebooted.

example% rem_drv -b /export/root/sun1 sd

SEE ALSO add_drv (1M), drvconfig (1M), kernel (1M)

1M-516 modified 18 Sep 1994